<LANGUAGE FOR="Packet Tracer 3.2">
	<NAME>English</NAME>
	<GUI>
		<SPLASH_SCREEN>
			<NV_GREET>Please wait...</NV_GREET>
			<NV_COPYRIGHT>© 2004 Cisco Systems, Inc.</NV_COPYRIGHT>
			<NV_LOADING>Loading...</NV_LOADING>
			<NV_SAVING>Saving...</NV_SAVING>
			<NV_INIT_NETWORK>Initializing network...</NV_INIT_NETWORK>
		</SPLASH_SCREEN>
		<TITLE_MENU>
			<FILE_MENU>
				<NV_FILE>File</NV_FILE>
				<NV_NEW>New</NV_NEW>
				<NV_OPEN>Open...</NV_OPEN>
				<NV_SAVE>Save</NV_SAVE>
				<NV_SAVE_AS>Save As...</NV_SAVE_AS>
				<NV_EXIT>Exit</NV_EXIT>
				<NV_PRINT>Print...</NV_PRINT>
				<NV_ACTIVITYEDITOR>Activity Wizard</NV_ACTIVITYEDITOR>
			</FILE_MENU>
			<OPTIONS_MENU>
				<NV_OPTIONS>Options</NV_OPTIONS>
				<NV_SIMPLE_MODE>Simple Mode</NV_SIMPLE_MODE>
				<NV_LANGUAGE>Language</NV_LANGUAGE>
				<NV_ANIMATION>Animation</NV_ANIMATION>
				<NV_SOUND>Sound</NV_SOUND>
				<NV_ZOOM_RADAR>Zoom Radar</NV_ZOOM_RADAR>
				<NV_AUTODHCP>Auto DHCP</NV_AUTODHCP>
				<NV_CHALLENGE_MODE>Challenge Mode</NV_CHALLENGE_MODE>
				<NV_CONSOLE_MODE>Console Mode</NV_CONSOLE_MODE>
				<NV_AUTOINFO>Show Packets</NV_AUTOINFO>
				<NV_AUTOPORTS>Hide Ports</NV_AUTOPORTS>
			</OPTIONS_MENU>
			<HELP_MENU>
				<NV_HELP>Help</NV_HELP>
				<NV_CONTENTS>Contents</NV_CONTENTS>
				<NV_TUTORIALS>Tutorials</NV_TUTORIALS>
				<NV_ABOUT>About</NV_ABOUT>
			</HELP_MENU>
			<MISC>
				<NV_CHECK_RESULTS>Check Results</NV_CHECK_RESULTS>
			</MISC>
		</TITLE_MENU>
		<PANELS>
			<TOPOLOGY>
				<NV_TAB_LABEL>Topology</NV_TAB_LABEL>
				<NV_B_ROUTER_ICON_LABEL>Router</NV_B_ROUTER_ICON_LABEL>
				<NV_B_CLOUD_ICON_LABEL>Cloud</NV_B_CLOUD_ICON_LABEL>
				<NV_B_SWITCH_ICON_LABEL>Switch</NV_B_SWITCH_ICON_LABEL>
				<NV_B_BRIDGE_ICON_LABEL>Bridge</NV_B_BRIDGE_ICON_LABEL>
				<NV_B_REPEATER_ICON_LABEL>Repeater</NV_B_REPEATER_ICON_LABEL>
				<NV_B_HUB_ICON_LABEL>Hub</NV_B_HUB_ICON_LABEL>
				<NV_B_ACCESS_POINT_ICON_LABEL>Access Point </NV_B_ACCESS_POINT_ICON_LABEL>
				<NV_B_PC_ICON_LABEL>PC</NV_B_PC_ICON_LABEL>
				<NV_B_CONNECTION_ICON_LABEL>Connect</NV_B_CONNECTION_ICON_LABEL>
				<NV_B_REMOVE_ICON_LABEL>Remove</NV_B_REMOVE_ICON_LABEL>
				<NV_B_SERVER_ICON_LABEL>Server</NV_B_SERVER_ICON_LABEL>
				<NV_B_PRINTER_ICON_LABEL>Printer</NV_B_PRINTER_ICON_LABEL>
				<NV_TOPOLOGYTABCAPTION>Enter Topology Mode</NV_TOPOLOGYTABCAPTION>
			</TOPOLOGY>
			<SIMULATION>
				<NV_TAB_LABEL>Simulation</NV_TAB_LABEL>
				<MOVIE_CONTROLS>
					<NV_TIME>TIME:</NV_TIME>
					<NV_MOVIEBACKWARDCAPTION>Step Backward</NV_MOVIEBACKWARDCAPTION>
					<NV_MOVIEFORWARDCAPTION>Step Forward</NV_MOVIEFORWARDCAPTION>
					<NV_MOVIEPAUSECAPTION>Pause Movie</NV_MOVIEPAUSECAPTION>
					<NV_MOVIEPLAYCAPTION>Play Movie</NV_MOVIEPLAYCAPTION>
					<NV_MOVIEENDCAPTION>Go to last step</NV_MOVIEENDCAPTION>
					<NV_MOVIEBEGCAPTION>Go to first step</NV_MOVIEBEGCAPTION>
					<NV_MOVIESLIDERCAPTION>Change movie speed</NV_MOVIESLIDERCAPTION>
				</MOVIE_CONTROLS>
				<SCENARIO>
					<NV_NEW>New</NV_NEW>
					<NV_DELETE>Delete</NV_DELETE>
					<NV_NEWPACKET>Create a new Packet</NV_NEWPACKET>
					<NV_CHANGEPACKETCOLORBTNCAPTION>Select a new packet color</NV_CHANGEPACKETCOLORBTNCAPTION>
					<NV_DELETEPACKETBTNCAPTION>Remove this packet</NV_DELETEPACKETBTNCAPTION>
					<NV_SCNEARIOINFOBOXCAPTION>Edit this scenario description</NV_SCNEARIOINFOBOXCAPTION>
					<NV_SCENARIO>Scenario </NV_SCENARIO>
					<NV_RIP_INIT>RIP Init</NV_RIP_INIT>
					<NV_RIP_INIT_DESCRIPTION>This special scenario demonstrates how RIP converges in this network.</NV_RIP_INIT_DESCRIPTION>
				</SCENARIO>
				<NV_SIMULATIONTABCAPTION>Enter Simulation Mode</NV_SIMULATIONTABCAPTION>

			</SIMULATION>
			<REALTIME>
				<NV_TAB_LABEL>Realtime</NV_TAB_LABEL>
				<PING_LOG>
					<NV_DESCRIPTION>Ping Log</NV_DESCRIPTION>
					<NV_SUCCESS_RATE_MSG>SUCCESSFUL</NV_SUCCESS_RATE_MSG>
					<NV_FAILED_MSG>FAILED</NV_FAILED_MSG>
					<NV_PINGBUTTON>Ping</NV_PINGBUTTON>
					<NV_PING_BUTTON_CAPTION>Ping a device</NV_PING_BUTTON_CAPTION>
				</PING_LOG>				
				<NV_REALTIMETABCAPTION>Enter Realtime Mode</NV_REALTIMETABCAPTION>				
			</REALTIME>
			<MODE_ICONS>
				<NV_SIMPLEMODECAPTION>Simple Mode Enabled</NV_SIMPLEMODECAPTION>
				<NV_CHALLENGEMODECAPTION>Challenge Mode Enabled</NV_CHALLENGEMODECAPTION>
				<NV_CONSOLEMODECAPTION>Console Mode Enabled</NV_CONSOLEMODECAPTION>
			</MODE_ICONS>
		</PANELS>
		<DIALOGS>
			<COMMON>
				<NV_YES_BTN>Yes</NV_YES_BTN>
				<NV_NO_BTN>No</NV_NO_BTN>
				<NV_CANCEL_BTN>Cancel</NV_CANCEL_BTN>
				<NV_OK_BTN>OK</NV_OK_BTN>
				<NV_CREATE_BTN>Create</NV_CREATE_BTN>
			</COMMON>
			<EDIT_DIALOGS>
				<TITLE_BAR>
					<NV_EDIT_DEVICE>Edit [[DEVICE_NAME]]</NV_EDIT_DEVICE>
					<NV_TERMINAL>[[DEVICE_NAME]] Terminal</NV_TERMINAL>
				</TITLE_BAR>
				<MAIN>
					<MAIN_CONFIG>
						<NV_ROUTER>Router Name:</NV_ROUTER>
						<NV_CLOUD>Cloud Name:</NV_CLOUD>
						<NV_SWITCH>Switch Name:</NV_SWITCH>
						<NV_BRIDGE>Bridge Name:</NV_BRIDGE>
						<NV_REPEATER>Repeater Name:</NV_REPEATER>
						<NV_HUB>Hub Name:</NV_HUB>
						<NV_ACCESS_POINT>Access Point Name:</NV_ACCESS_POINT>
						<NV_PC>PC Name:</NV_PC>
						<NV_SERVER>Server Name:</NV_SERVER>
						<NV_PRINTER>Printer Name:</NV_PRINTER>
						<NV_POWER>Power</NV_POWER>
						<NV_ON>On</NV_ON>
						<NV_OFF>Off</NV_OFF>
						<NV_DHCP_SERVER>DHCP Server:</NV_DHCP_SERVER>
						<NV_ENABLE_DHCP>Enable</NV_ENABLE_DHCP>
						<NV_DISABLE_DHCP>Disable</NV_DISABLE_DHCP>
						<NV_AUTO_CONFIG>Auto Config</NV_AUTO_CONFIG>
						<NV_GATEWAY>Gateway:</NV_GATEWAY>
						<NV_SELECT_PORT>Select Port:</NV_SELECT_PORT>
						<NV_PORT_CONFIG>Port Config</NV_PORT_CONFIG>
						<NV_ROUTING_CONFIG>Static Routing</NV_ROUTING_CONFIG>
						<NV_NOTE>Note: Configurations (if valid) are saved as soon as they are made or changed.</NV_NOTE>
						<NV_DYNAMIC_ROUTING>Dynamic Routing</NV_DYNAMIC_ROUTING>
						<NV_AUTODYNAMIC>Automatic</NV_AUTODYNAMIC>
						<NV_TRANSMISSION_DELAY>Transmission Delay:</NV_TRANSMISSION_DELAY>
						<NV_NV_RAM>NV RAM:</NV_NV_RAM>
						<NV_VLAN_DATABASE>VLAN Database</NV_VLAN_DATABASE>
						<NV_TERMINAL>Terminal</NV_TERMINAL>
						<NV_Cmd_Prompt>Cmd Prompt</NV_Cmd_Prompt>
					</MAIN_CONFIG>
					<SLOT_MENU>
						<NV_COPPER_ETHERNET>Copper Ethernet</NV_COPPER_ETHERNET>
						<NV_COPPER_FAST_ETHERNET>Copper Fast Ethernet</NV_COPPER_FAST_ETHERNET>
						<NV_COPPER_GIG_ETHERNET>Copper Gigabit Ethernet</NV_COPPER_GIG_ETHERNET>
						<NV_FIBER_FAST_ETHERNET>Fiber Fast Ethernet</NV_FIBER_FAST_ETHERNET>
						<NV_FIBER_GIG_ETHERNET>Fiber Gigabit Ethernet</NV_FIBER_GIG_ETHERNET>
						<NV_SERIAL>Serial</NV_SERIAL>
						<NV_MODEM>Modem</NV_MODEM>
						<NV_WIRELESS>Wireless</NV_WIRELESS>
						<NV_CONSOLE>Console</NV_CONSOLE>
						<NV_RS_232>RS 232</NV_RS_232>
						<NV_VLAN>Vlan</NV_VLAN>
					</SLOT_MENU>
					<PORT_CONFIG>
						<NV_ON>On</NV_ON>
						<NV_OFF>Off</NV_OFF>
						<NV_REMOVE>Remove</NV_REMOVE>
						<NV_PORT_STATUS>Port Status:</NV_PORT_STATUS>
						<NV_BANDWIDTH>Bandwidth:</NV_BANDWIDTH>
						<NV_DUPLEX>Duplex:</NV_DUPLEX>
						<NV_MAC_ADDRESS>MAC Address:</NV_MAC_ADDRESS>
						<NV_IP_ADDRESS>IP Address:</NV_IP_ADDRESS>
						<NV_SUBNET_MASK>Subnet Mask:</NV_SUBNET_MASK>
						<NV_CLOCKING>Clocking:</NV_CLOCKING>
						<NV_SWITCH_MODE>Switch Mode:</NV_SWITCH_MODE>
						<NV_AUTO_NEGO>Auto Negotiate</NV_AUTO_NEGO>
						<NV_10MBPS>10 Mbps</NV_10MBPS>
						<NV_100MBPS>100 Mbps</NV_100MBPS>
						<NV_1000MBPS>1000 Mbps</NV_1000MBPS>
						<NV_56KBPS>56 Kbps</NV_56KBPS>
						<NV_128KBPS>128 Kbps</NV_128KBPS>
						<NV_384KBPS>384 Kbps</NV_384KBPS>
						<NV_768KBPS>768 Kbps</NV_768KBPS>
						<NV_1544KBPS>1.544 Mbps</NV_1544KBPS>
						<NV_2048KBPS>2.048 Mbps</NV_2048KBPS>
						<NV_11Mbps>11 Mbps</NV_11Mbps>
						<NV_ENABLE_CLOCKING>Enable</NV_ENABLE_CLOCKING>
						<NV_DISABLE_CLOCKING>Disable</NV_DISABLE_CLOCKING>
						<NV_DUPLEX_FULL>Full Duplex</NV_DUPLEX_FULL>
						<NV_DUPLEX_HALF>Half Duplex</NV_DUPLEX_HALF>
						<NV_DUPLEX_AUTO>Auto Negotiate</NV_DUPLEX_AUTO>
						<NV_ACCESS_VLAN>Access VLAN:</NV_ACCESS_VLAN>
						<NV_TRUNK_VLAN>Trunk VLANs:</NV_TRUNK_VLAN>
						<NV_USE_DHCP>Use DHCP</NV_USE_DHCP>
					</PORT_CONFIG>
					<ROUTING_CONFIG>
						<NV_GATEWAY>Gateway of Last Resort:</NV_GATEWAY>
						<NV_STATIC_ROUTES>Static Routes</NV_STATIC_ROUTES>
						<NV_NETWORK>Network</NV_NETWORK>
						<NV_MASK>Mask</NV_MASK>
						<NV_NEXT_HOP>Next Hop</NV_NEXT_HOP>
						<NV_ADD>Add</NV_ADD>
						<NV_REMOVE>Remove</NV_REMOVE>
						<NV_ENTRY>[[NETWORK]]/[[MASK_BITS]] via [[NEXT_HOP]]</NV_ENTRY>
						<NV_SAVE_NVRAM>Save NV RAM</NV_SAVE_NVRAM>
						<NV_ERASE_NVRAM>Erase NV RAM</NV_ERASE_NVRAM>
					</ROUTING_CONFIG>
					<CONSOLE_CONFIG>
						<NV_SPEED>Speed:</NV_SPEED>
						<NV_BITS_PER_SECOND>Bits Per Second:</NV_BITS_PER_SECOND>
						<NV_DATA_BITS>Data Bits:</NV_DATA_BITS>
						<NV_PARITY>Parity:</NV_PARITY>
						<NV_STOP_BITS>Stop Bits:</NV_STOP_BITS>
						<NV_FLOW_CONTROL>Flow Control:</NV_FLOW_CONTROL>
						<NV_PARITY_EVEN>Even</NV_PARITY_EVEN>
						<NV_PARITY_ODD>Odd</NV_PARITY_ODD>
						<NV_PARITY_NONE>None</NV_PARITY_NONE>
						<NV_PARITY_MARK>Mark</NV_PARITY_MARK>
						<NV_PARITY_SPACE>Space</NV_PARITY_SPACE>
						<NV_FC_SOFTWARE>Software</NV_FC_SOFTWARE>
						<NV_FC_XON_XOFF>Xon/Xoff</NV_FC_XON_XOFF>
						<NV_FC_HARDWARE>Hardware</NV_FC_HARDWARE>
						<NV_FC_NONE>None</NV_FC_NONE>
						<NV_OPEN_TERMINAL>Open Terminal</NV_OPEN_TERMINAL>

					</CONSOLE_CONFIG>
					<VLAN_DATABASE>
						<NV_VLAN_NUMBER>VLAN Number:</NV_VLAN_NUMBER>
						<NV_VLAN_NAME>VLAN Name:</NV_VLAN_NAME>
					</VLAN_DATABASE>
				</MAIN>
			</EDIT_DIALOGS>
			<SAVE_DIALOG>
				<NV_TITLE>Save?</NV_TITLE>
				<NV_BODY_MSG>Do you want to save?</NV_BODY_MSG>
			</SAVE_DIALOG>
			<DELETE_PC>
				<NV_TITLE>Delete [[DEVICE_TYPE]]?</NV_TITLE>
				<NV_BODY_MSG>All packets sent from this [[DEVICE_TYPE]] will also be deleted. Continue with delete?</NV_BODY_MSG>
			</DELETE_PC>
			<ERROR_MSG>
				<FRAME_DIALOG>
					<NV_IP_INVALID>The IP Address is invalid. Please enter another IP Address.</NV_IP_INVALID>
					<NV_MAC_INVALID>The MAC Address is invalid. Please enter another MAC address.</NV_MAC_INVALID>
					<NV_TTL_INVALID>The Time to Live (TTL) is invalid. Please enter a number between 0 and 255.</NV_TTL_INVALID>
					<NV_SRC_PORT_INVALID>The source port is invalid. Please enter a number between 1 and 65535.</NV_SRC_PORT_INVALID>
					<NV_DST_PORT_INVALID>The destination port is invalid. Please enter a number between 1 and 65535.</NV_DST_PORT_INVALID>
					<NV_SEQUENCE_NUMBER_INVALID>The sequence number is invalid. Please enter a number between 0 and 65535.</NV_SEQUENCE_NUMBER_INVALID>
				</FRAME_DIALOG>
				<EDIT_DIALOGS>
					<NV_GATEWAY_INVALID>The gateway address is invalid. Please enter another gateway address.</NV_GATEWAY_INVALID>
					<NV_GATEWAY_IP_EXIST>The gateway address is the same as Port [[PORT#]]'s IP address. Please enter a next hop address.</NV_GATEWAY_IP_EXIST>
					<NV_DHCP_NOT_FOUND>DHCP server (router) not found. Please connect this [[DEVICE_TYPE]] to a router first.</NV_DHCP_NOT_FOUND>
					<NV_IP_INVALID>The IP address is invalid. Please enter another IP address.</NV_IP_INVALID>
					<NV_SUBNET_INVALID>The subnet mask is a bad mask for the IP address. Please enter another subnet mask.</NV_SUBNET_INVALID>
					<NV_PORT_EXIST>Duplicate IP address on [[PORTTYPE]] [[PORT#]] of [[DEVICE]]. Please enter another IP address.</NV_PORT_EXIST>
					<NV_IP_WRONG_SUBNET>The IP address is in the same subnet as another port on this device. Please enter another IP address.</NV_IP_WRONG_SUBNET>
					<NV_INCOMPLETE_PORT_CONFIG>The IP and subnet mask configuration on Port [[PORT#]] is incomplete. Please return to Port [[PORT#]] and complete the configuration</NV_INCOMPLETE_PORT_CONFIG>
					<NV_NETWORK_INVALID>The Network field is invalid. Please enter another network.</NV_NETWORK_INVALID>
					<NV_MASK_INVALID>The Mask field is invalid. Please enter another mask.</NV_MASK_INVALID>
					<NV_NEXT_HOP_INVALID>The Next Hop field is invalid. Please enter another next hop address.</NV_NEXT_HOP_INVALID>
					<NV_NEXT_HOP_EXIST>The Next Hop address is the same as Port [[PORT#]]'s IP address. Please enter a next hop address.</NV_NEXT_HOP_EXIST>
					<NV_AUTO_DYNAMIC_ENABLED>Automatic dynamic routing is enabled. Disable it to manually configure dynamic routing networks.</NV_AUTO_DYNAMIC_ENABLED>
					<NV_VLAN_INVALID>The new VLAN's number is invalid. Please enter a number between 2 and 1005.</NV_VLAN_INVALID>
					<NV_MAC_INVALID>Invalid MAC Address. The proper format is: XXXX.XXXX.XXXX. Allowed Characters: 0-9, A-F</NV_MAC_INVALID>
					<NV_DUPE_MAC>Duplicate MAC address on [[PORTTYPE]] [[PORT#]] of [[DEVICE]]. Please enter another MAC address.</NV_DUPE_MAC>
					<NV_MAC_MALFORMED>Malformed hex mac address</NV_MAC_MALFORMED>
					<NV_HOSTNAMENOTUNIQUE>The hostname is not unique. Please enter an unique hostname.</NV_HOSTNAMENOTUNIQUE>
					<NV_INVALIDHOSTNAME>The hostname must be at least one character in length.</NV_INVALIDHOSTNAME>
				</EDIT_DIALOGS>
				<FILE_MANAGER>
					<NV_FILE_INVALID>This file is not a valid Packet Tracer [[VERSION]] file. Please select another file.</NV_FILE_INVALID>
				</FILE_MANAGER>
				<WORKSPACE_TOPOLOGY>
					<NV_SAME_DEVICE_CONNECT_NOT_ALLOWED>A device cannot make a connection to itself. Please select another device.</NV_SAME_DEVICE_CONNECT_NOT_ALLOWED>
					<NV_CONNECTION_FAILED>A connection cannot be made between [[SRCDEVICE]] and [[DSTDEVICE]]. Please select another device.</NV_CONNECTION_FAILED>
				</WORKSPACE_TOPOLOGY>
				<WORKSPACE_SIMULATION>
					<NV_NO_FUNC_PORTS>The [[DEVICE_TYPE]] does not have any functional ports. Please select another device.</NV_NO_FUNC_PORTS>
					<NV_ONE_FRAME_AT_A_TIME>A [[DEVICE_TYPE]] can send only one packet at a time. Please select another host.</NV_ONE_FRAME_AT_A_TIME>
					<NV_NO_SEND_TO_SELF>A [[DEVICE_TYPE]] cannot send packets to itself. Please select another host.</NV_NO_SEND_TO_SELF>
				</WORKSPACE_SIMULATION>
				<WORKSPACE_REALTIME>
					<NV_NOIPONHOST>This device does not have any IP Addresses configured.</NV_NOIPONHOST>	
				</WORKSPACE_REALTIME>
				<LOCK_ARBITER>
					<NV_TOPOLOGY>Switching to Topology mode has been disabled.</NV_TOPOLOGY>
					<NV_SIMULATION>Switching to Simulation mode has been disabled.</NV_SIMULATION>
					<NV_REALTIME>Switching to Realtime mode has been disabled.</NV_REALTIME>
					<NV_SIMPLE>Toggling Simple mode has been disabled.</NV_SIMPLE>
					<NV_CONSOLE>Toggling Console mode has been disabled.</NV_CONSOLE>
					<NV_CHALLENGE>Toggling Challenge mode has been disabled.</NV_CHALLENGE>
					<NV_ANIMATION>Toggling Animation has been disabled.</NV_ANIMATION>
					<NV_SOUND>Toggling Sound has been disabled.</NV_SOUND>
					<NV_SHOWPACKETS>Toggling Show Packets has been disabled.</NV_SHOWPACKETS>
					<NV_HIDEPORTS>Toggling Hide Ports has been disabled.</NV_HIDEPORTS>
					<NV_ZOOMRADAR>Toggling Zoom Radar has been disabled.</NV_ZOOMRADAR>
					<NV_AUTODHCP>Toggling Auto DHCP has been disabled.</NV_AUTODHCP>
					<NV_LANGUAGE>Toggling Language has been disabled.</NV_LANGUAGE>
					<NV_CREATEDEVICES>Creating devices has been disabled.</NV_CREATEDEVICES>
					<NV_REMOVEDEVICES>Removing devices has been disabled.</NV_REMOVEDEVICES>
					<NV_REMOVEALLDEVICES>Removing devices has been disabled on one or more devices. Please deselect those devices and try again.</NV_REMOVEALLDEVICES>
					<NV_POWER>Toggling Power has been disabled.</NV_POWER>
					<NV_CONFIG>Configuration has been disabled.</NV_CONFIG>
					<NV_ADDPORT>Adding or Changing interfaces has been disabled.</NV_ADDPORT>
					<NV_REMOVEPORT>Removing interfaces has been disabled.</NV_REMOVEPORT>
					<NV_CONNECTLINKS>Connecting links has been disabled.</NV_CONNECTLINKS>
					<NV_DISCONNECTLINKS>Disconnecting links has been disabled.</NV_DISCONNECTLINKS>
					<NV_CREATESCENARIOS>Creating scenarios has been disabled.</NV_CREATESCENARIOS>
					<NV_REMOVESCENARIOS>Removing scenarios has been disabled.</NV_REMOVESCENARIOS>
					<NV_RENAMESCENARIOS>Renaming scenarios has been disabled.</NV_RENAMESCENARIOS>
					<NV_CREATEPACKETS>Creating packets has been disabled.</NV_CREATEPACKETS>
					<NV_REMOVEPACKETS>Removing packets has been disabled.</NV_REMOVEPACKETS>
				</LOCK_ARBITER>
				<SCENARIO>
					<NV_SCENARIONAMENOTUNIQUE>The scenario name is not unique. Please enter a unique scenario name</NV_SCENARIONAMENOTUNIQUE>
					<NV_NOCHANGESPECIALSCENARIO>This action is not allowed for special scenarios.</NV_NOCHANGESPECIALSCENARIO>
				</SCENARIO>
			</ERROR_MSG>
			<ADD_FRAME_DIALOG>
				<NV_TITLE>Create Packet/Frame</NV_TITLE>
				<NV_FRAME_CONFIG>Frame Config</NV_FRAME_CONFIG>
				<NV_SELECT_DST_MSG>Select a destination host or enter its address(es): </NV_SELECT_DST_MSG>
				<NV_IP>IP Address:</NV_IP>
				<NV_MAC>MAC Address:</NV_MAC>
				<NV_USE_ARP>Use ARP</NV_USE_ARP>
				<NV_BROADCAST>Broadcast</NV_BROADCAST>
				<NV_PACKET_CONFIG>Packet Config</NV_PACKET_CONFIG>
				<NV_TTL>TTL:</NV_TTL>
				<NV_DEFINING>Defining...</NV_DEFINING>
				<NV_IPPROTOCOL>IP Protocol</NV_IPPROTOCOL>
				<NV_SEGMENT_CONFIG>Segment Config</NV_SEGMENT_CONFIG>
				<NV_APPLICATION>Application:</NV_APPLICATION>
				<NV_APPLICATIONCUSTOM>Other</NV_APPLICATIONCUSTOM>
				<NV_SRCPORT>Source Port:</NV_SRCPORT>
				<NV_DSTPORT>Destination Port:</NV_DSTPORT>
				<NV_SEQUENCE_NUMBER>Sequence Number:</NV_SEQUENCE_NUMBER>
			</ADD_FRAME_DIALOG>
			<ROUTING_TABLE>
				<NV_TITLE>Routing Table for </NV_TITLE>
				<NV_TYPE>Type</NV_TYPE>
				<NV_NETWORK>Network</NV_NETWORK>
				<NV_PORT>Port</NV_PORT>
				<NV_NEXT_HOP_IP>Next Hop IP</NV_NEXT_HOP_IP>
				<NV_METRIC>Metric</NV_METRIC>
			</ROUTING_TABLE>
			<MAC_TABLE>
				<NV_TITLE>MAC Table for </NV_TITLE>
				<NV_VLAN>VLAN</NV_VLAN>
				<NV_MAC_ADDRESS>MAC Address</NV_MAC_ADDRESS>
				<NV_PORT>Port</NV_PORT>
			</MAC_TABLE>
			<PACKET_INFO>
				<NV_TITLE>Packet Info at Device: </NV_TITLE>
				<NV_SEE_ANSWERS>Check Answers</NV_SEE_ANSWERS>
				<NV_MY_ANSWERS>My Answers</NV_MY_ANSWERS>
			</PACKET_INFO>
			<PORT_SELECT_MENU>
				<NV_TITLE>Port Select</NV_TITLE>
			</PORT_SELECT_MENU>
			<DEVICE_TYPE>
				<NV_PC>PC</NV_PC>
				<NV_SERVER>server</NV_SERVER>
				<NV_PRINTER>printer</NV_PRINTER>
				<NV_ROUTER>router</NV_ROUTER>
				<NV_CLOUD>cloud</NV_CLOUD>
			</DEVICE_TYPE>
			<INFO_DIALOG>
				<NV_TITLE>[[OBJECT NAME]] Description</NV_TITLE>
				<NV_NETWORK_DESCRIPTION>Network Description</NV_NETWORK_DESCRIPTION>
				<NV_INFOLOCK>
					<NV_LOCK_TITLE>Lock Information</NV_LOCK_TITLE>
					<NV_UNLOCK_TITLE>Unlock Information</NV_UNLOCK_TITLE>
					<NV_PASSWORD>Password:</NV_PASSWORD>
					<NV_CONFIRM_PASSWORD>Confirm Password:</NV_CONFIRM_PASSWORD>
					<NV_LOCK>Lock Information Box?</NV_LOCK>
					<NV_UNLOCK>Unlock Information Box?</NV_UNLOCK>
					<NV_MISMATCH_PASSWORD>Password does not match.</NV_MISMATCH_PASSWORD>
					<NV_INCORRECT_PASSWORD>Incorrect Password.</NV_INCORRECT_PASSWORD>
					<NV_LOCKOPENCAPTION>Lock the information box</NV_LOCKOPENCAPTION>
					<NV_LOCKCLOSECAPTION>Unlock the information box</NV_LOCKCLOSECAPTION>
					<NV_ENABLEPASSWORD>Enable Password</NV_ENABLEPASSWORD>
					<NV_DISABLEPASSWORD>Disable Password</NV_DISABLEPASSWORD>
				</NV_INFOLOCK>
			</INFO_DIALOG>
			<DELETE_SELECTED>
				<NV_TITLE>Delete Devices?</NV_TITLE>
				<NV_BODY_MSG>Deleting devices cannot be undone. Continue with delete?</NV_BODY_MSG>
			</DELETE_SELECTED>
			<NEW_DIALOG>
				<NV_TITLE>New network</NV_TITLE>
				<NV_BODY_MSG>Do you want to save before creating a new network?</NV_BODY_MSG>
			</NEW_DIALOG>
			<Open_DIALOG>
				<NV_TITLE>Open network</NV_TITLE>
				<NV_BODY_MSG>Do you want to save before opening another network?</NV_BODY_MSG>
			</Open_DIALOG>
		</DIALOGS>
		<LINK>
			<NV_CONNECTION_TYPE>Connection Type</NV_CONNECTION_TYPE>
			<NV_COPPER_STRAIGHT>Copper Straight-through</NV_COPPER_STRAIGHT>
			<NV_COPPER_CROSSOVER>Copper Cross-over</NV_COPPER_CROSSOVER>
			<NV_SERIAL>Serial</NV_SERIAL>
			<NV_DCE_SERIAL>Serial DCE</NV_DCE_SERIAL>
			<NV_DTE_SERIAL>Serial DTE</NV_DTE_SERIAL>
			<NV_FIBER>Fiber</NV_FIBER>
			<NV_WIRELESS>Wireless</NV_WIRELESS>
			<NV_PHONE>Phone</NV_PHONE>
			<NV_CONSOLE>Console</NV_CONSOLE>
		</LINK>
		<CANCEL_BUTTON>
			<NV_CANCEL>CANCEL</NV_CANCEL>
		</CANCEL_BUTTON>
		<MOUSE_OVER_DEVICE_INFO>
			<NV_PORT>Port</NV_PORT>
			<NV_LINK>Link</NV_LINK>
			<NV_IP>IP Address</NV_IP>
			<NV_MAC>MAC Address</NV_MAC>
			<NV_VLAN>VLAN</NV_VLAN>
			<NV_UP>Up</NV_UP>
			<NV_DOWN>Down</NV_DOWN>
			<NV_IP_NOT_SET>&lt;not set&gt;</NV_IP_NOT_SET>
			<NV_WAN_PORT>&lt;WAN address&gt;</NV_WAN_PORT>
			<NV_DEFAULT_GATEWAY>Default Gateway:</NV_DEFAULT_GATEWAY>
			<NV_GATEWAY_NOT_SET>&lt;not set&gt;</NV_GATEWAY_NOT_SET>
			<NV_GATEWAY_OF_LAST_RESORT>Gateway Of Last Resort:</NV_GATEWAY_OF_LAST_RESORT>			
		</MOUSE_OVER_DEVICE_INFO>
		<ACTIVITY>			
                                            <PROMPTS>
                                            	<COMMON>
                                            		 <NV_YES>Yes</NV_YES>
                                            		<NV_NO>No</NV_NO>
                                            		<NV_CONFRIM>Confirm</NV_CONFRIM>
                                            		<NV_CANCEL>Cancel</NV_CANCEL>
                                            	</COMMON>
                                            	<CONVERT_TO_ANSNET>
                                                           	<NV_TITLE>Convert to Answer Network?</NV_TITLE>
                                                           	<NV_MSG>Do you want to use the existing network as the Answer Network?</NV_MSG>
                                            	</CONVERT_TO_ANSNET>
                                            	<COPY_FROM_ANS_NET>
                                            		<NV_TITLE>Copy Network?</NV_TITLE>
                                            		<NV_MSG>Replacing the Initial Network with the Answer Network cannot be undone.</NV_MSG>
                                            	</COPY_FROM_ANS_NET>
                                            	<EXIT_ACTIVITY>
                                            		<NV_TITLE>Exit Activity Wizard?</NV_TITLE>
                                            		<NV_MSG>Exiting the Activity Wizard will give you a new workspace. All unsaved settings will be lost. Do you want to exit?</NV_MSG>
                                            	</EXIT_ACTIVITY>
                                            	<PASSWORD>
                                            		<NV_TITLE>Enter the Password: </NV_TITLE>
                                            		<NV_MSG>Please enter the password: </NV_MSG>
                                            		<NV_INVALID>Invalid Password</NV_INVALID>
                                            	</PASSWORD>
						<RESET_ACTIVITY>
							<NV_TITLE>Reset Activity?</NV_TITLE>
							<NV_MSG>Do you want to reset the activity? All configuration will be reset.</NV_MSG>
						</RESET_ACTIVITY>
                                            </PROMPTS>
			<WIZARD>
				<TITLES>
					<NV_MAIN>Activity Wizard</NV_MAIN>
					<NV_INIT>Activity Wizard - Initial Network</NV_INIT>
					<NV_ANS>Activity Wizard - Answer Network</NV_ANS>
					<NV_TEST>Activity Wizard - Test Activity</NV_TEST>					
				</TITLES>
				<NAVIGATION_PANEL>
					<NV_WELCOME>Welcome</NV_WELCOME>		                        
					<NV_INSTRUCTIONS>Instructions</NV_INSTRUCTIONS>
					<NV_ANSNETWORK>Answer Network</NV_ANSNETWORK>
					<NV_INITNETWORK>Initial Network</NV_INITNETWORK>
					<NV_PASSWORD>Password</NV_PASSWORD>
					<NV_TESTACTIVITY>Test Activity</NV_TESTACTIVITY>
					<NV_SAVE>Save</NV_SAVE> 
					<NV_EXIT>Exit</NV_EXIT>
				</NAVIGATION_PANEL>	
                                             	
				<WELCOME_CONTENT>
					<NV_MSG><![CDATA[<b>Welcome to the Activity Wizard!<br><br>The Activity Wizard is an assessment tool that allows you to create detailed networking scenarios for other users. The typical sequence in making an activity is as follows:<br><br>1) Create the Answer Network and decide the assessment items.<br>2) Create the Initial Network, which will be the user's starting point.<br>3) Put constraints on the user's freedom to use certain features during the activity.<br>4) Write a clear set of instructions for the activity.<br>5) Password protect the activity to prevent unauthorized changes to activity parameters.<br>6) Save the activity.<br><br>Please refer to the help files for the Activity Wizard for more detailed information.<br>]]></NV_MSG>
				</WELCOME_CONTENT>
				
				<INSTRUCTIONS_CONTENT>
					<NV_HEADER>Activity Instructions:</NV_HEADER>
					<NV_DIRECTIONS>Use the textfield below to enter the instructions for this activity.</NV_DIRECTIONS>
				</INSTRUCTIONS_CONTENT>
				
				<ANSWERNET_CONTENT>
					<LABELS>
						<NV_BUILDANSNET>Building Answer Network</NV_BUILDANSNET>
						<NV_EXPORTING>Exporting</NV_EXPORTING>
						<NV_SETASSESSMENTOPT>Set Assessment Options</NV_SETASSESSMENTOPT>
						<NV_SETASSESSMENTDIR>Use the tree below to select the components you want to assess. You may also use the View Filter to hide or show certain categories.</NV_SETASSESSMENTDIR>
						<NV_VIEWFILTER>View Filter</NV_VIEWFILTER>
						<NV_SHOWANSNETBTN>Show Answer Network</NV_SHOWANSNETBTN>
						<NV_EXPORTANSNETBTN>Export Answer Network</NV_EXPORTANSNETBTN>
						<NV_CHKIP>IP</NV_CHKIP> 
						<NV_CHKROUTING>Routing</NV_CHKROUTING> 
						<NV_CHKACL>ACL</NV_CHKACL> 
						<NV_CHKNAT>NAT</NV_CHKNAT> 
						<NV_CHKPHYS>Physical</NV_CHKPHYS> 
						<NV_CHKSWITCH>Switching</NV_CHKSWITCH> 
						<NV_CHKCONN>Connectivity</NV_CHKCONN>
						<NV_CHKVIEW>View/Hide All</NV_CHKVIEW>
					</LABELS>
					<COMPARATOR_TREE>
						<NV_PORTS>Ports</NV_PORTS>
						<NV_EXTACL>Extended Access-list [[ACL_ID]]</NV_EXTACL>
						<NV_STDACL>Standard Access-list [[ACL_ID]]</NV_STDACL>
						<NV_HOSTNAME>Host Name</NV_HOSTNAME>
						<NV_POWER>Power</NV_POWER>
						<NV_LINKTO>Link To [[DST_DEVICENAME]]</NV_LINKTO>
						<NV_TYPE>Type</NV_TYPE>
						<NV_CONNECTSTO>Connects to [[DST_PORT]]</NV_CONNECTSTO>
						<NV_DCE>DCE</NV_DCE>
						<NV_NETWORK>Network</NV_NETWORK>
						<NV_DEFAULTGATEWAY>Default Gateway</NV_DEFAULTGATEWAY>
						<NV_VLANINTERFACE>VLAN Interface [[PORT_NUM]]</NV_VLANINTERFACE>
						<NV_PORTNUM>Port [[PORT_NUM]]</NV_PORTNUM>
						<NV_PORTTYPE>Port Type</NV_PORTTYPE>
						<NV_DESCRIPTION>Description</NV_DESCRIPTION>
						<NV_MAC>MAC Address</NV_MAC>
						<NV_BANDWIDTH>Bandwidth</NV_BANDWIDTH>
						<NV_DUPLEX>Duplex</NV_DUPLEX>
						<NV_CLOCKENABLED>Clock Enabled</NV_CLOCKENABLED>
						<NV_CLOCKRATE>Clock Rate</NV_CLOCKRATE>
						<NV_CDPENABLED>CDP Enabled</NV_CDPENABLED>
						<NV_IP>IP Address</NV_IP>
						<NV_SUBNET>Subnet Mask</NV_SUBNET>
						<NV_ACLGIN>Access-group In</NV_ACLGIN>
						<NV_ACLGOUT>Access-group Out</NV_ACLGOUT>
						<NV_NAT>NAT</NV_NAT>
						<NV_TRANSDELAY>Transmission Delay</NV_TRANSDELAY>
						<NV_DHCPENABLED>DHCP Enabled</NV_DHCPENABLED>
						<NV_CDPRUN>CDP Run</NV_CDPRUN>
						<NV_STATICROUTES>Static Routes</NV_STATICROUTES>
						<NV_AUTODR>Automatic Dynamic Routing</NV_AUTODR>
						<NV_RIP>RIP</NV_RIP>
						<NV_VERSION>Version</NV_VERSION>
						<NV_AUTOSUM>Auto Summary</NV_AUTOSUM>
						<NV_PASSIVEINT>Passive Interface</NV_PASSIVEINT>
						<NV_DEFAULT>default</NV_DEFAULT>
						<NV_NETWORKS>Networks</NV_NETWORKS>
						<NV_ACLS>Access-lists</NV_ACLS>
						<NV_NATPOOL>NAT pool</NV_NATPOOL>
						<NV_INSTATICNAT>Inside Source Static NAT</NV_INSTATICNAT>
						<NV_INLISTNAT>Inside Source List NAT</NV_INLISTNAT>
						<NV_STARTCONFIG>Startup Config</NV_STARTCONFIG>
						<NV_RS232>RS232</NV_RS232>
						<NV_SPEED>Speed</NV_SPEED>
						<NV_DATABITS>Databits</NV_DATABITS>
						<NV_PARITY>Parity</NV_PARITY>
						<NV_STOPBITS>Stop Bits</NV_STOPBITS>
						<NV_FLOWCONTROL>Flow Control</NV_FLOWCONTROL>
						<NV_VLANS>VLANs</NV_VLANS>
						<NV_VLANINTERFACES>VLAN Interfaces</NV_VLANINTERFACES>
						<NV_SWITCHPORTMODE>Switchport Mode</NV_SWITCHPORTMODE>
						<NV_ACCESSVLAN>Access VLAN</NV_ACCESSVLAN>
						<NV_TRUNKVLAN>Trunk VLANs</NV_TRUNKVLAN>
						<NV_CONSOLE>Console</NV_CONSOLE>
						<NV_VLANNUM>VLAN [[VLAN_NUM]]</NV_VLANNUM>
						<NV_VLANNAME>VLAN Name</NV_VLANNAME>
						<NV_PORTSECURITY>Port Security</NV_PORTSECURITY>
						<NV_ENABLED>Enabled</NV_ENABLED>
						<NV_MAXSECUREADDR>Max Secure Addresses</NV_MAXSECUREADDR>
						<NV_VIOLATIONMODE>Violation Mode</NV_VIOLATIONMODE>
						<NV_SECUREMACADDR>Secure MAC Addresses</NV_SECUREMACADDR>
						<NV_PORTERRDISABLED>Port Error Disabled</NV_PORTERRDISABLED>						
					</COMPARATOR_TREE>
				</ANSWERNET_CONTENT>					
				<INITIALNET_CONTENT>
					<LABELS>
						<NV_BUILDINITNET>Building Initial Network</NV_BUILDINITNET>
						<NV_EXPORTING>Exporting</NV_EXPORTING>
						<NV_SETLOCKOPTIONS>Set the Locking Options</NV_SETLOCKOPTIONS>
						<NV_SETLOCKOPTIONSDIR>Use the locking tree below to lock out certain functions for this activity when it is run.</NV_SETLOCKOPTIONSDIR>
						<NV_COPYANSNETBTN>Copy From Answer Network</NV_COPYANSNETBTN>
						<NV_SHOWINITNETBTN>Show Initial Network</NV_SHOWINITNETBTN>
						<NV_EXPORTINITNETBTN>Export Initial Network</NV_EXPORTINITNETBTN>		
					</LABELS>
					<LOCKING_TREE>
						<NV_LOCKING>Locking</NV_LOCKING>
						<NV_INTERFACE>Interface</NV_INTERFACE>
						<NV_SWITCHINGTOTOPOLOGY>Switching to Topology</NV_SWITCHINGTOTOPOLOGY>
						<NV_SWITCHINGTOSIMULATION>Switching to Simulation</NV_SWITCHINGTOSIMULATION>
						<NV_SWITCHINGTOREALTIME>Switching to Realtime</NV_SWITCHINGTOREALTIME>
						<NV_MODES>Modes</NV_MODES>
						<NV_SWITCHINGTOSIMPLE>Toggle Simple</NV_SWITCHINGTOSIMPLE>
						<NV_SWITCHINGTOCONSOLE>Toggle Console</NV_SWITCHINGTOCONSOLE>
						<NV_SWITCHINGTOCHALLENGE>Toggle Challenge</NV_SWITCHINGTOCHALLENGE>
						<NV_PREFERENCES>Preferences</NV_PREFERENCES>
						<NV_ANIMATION>Toggle Animation</NV_ANIMATION>
						<NV_SOUND>Toggle Sound</NV_SOUND>
						<NV_SHOWPACKETS>Toggle Show Packets</NV_SHOWPACKETS>
						<NV_HIDEPORTS>Toggle Hide Ports</NV_HIDEPORTS>
						<NV_ZOOMRADAR>Toggle Zoom Radar</NV_ZOOMRADAR>
						<NV_AUTODHCP>Toggle Auto DHCP</NV_AUTODHCP>
						<NV_LANGUAGE>Change Language</NV_LANGUAGE>
						<NV_TOPOLOGY>Topology</NV_TOPOLOGY>
						<NV_GLOBAL>Global</NV_GLOBAL>
						<NV_CREATEDEVICES>Create Devices</NV_CREATEDEVICES>
						<NV_REMOVEDEVICES>Remove Devices</NV_REMOVEDEVICES>
						<NV_CREATELINKS>Connect Links</NV_CREATELINKS>
						<NV_REMOVELINKS>Disconnect Links</NV_REMOVELINKS>
						<NV_POWER>Toggle Power</NV_POWER>
						<NV_CONFIGVIADIALOG>Configuration</NV_CONFIGVIADIALOG>
						<NV_EXISTINGDEVICES>Existing Devices</NV_EXISTINGDEVICES>
						<NV_EXISTINGLINKS>Existing Links</NV_EXISTINGLINKS>
						<NV_SIMULATION>Simulation</NV_SIMULATION>
						<NV_CREATESCENARIOS>Create Scenarios</NV_CREATESCENARIOS>
						<NV_REMOVESCENARIOS>Remove Scenarios</NV_REMOVESCENARIOS>
						<NV_RENAMESCENARIOS>Rename Scenarios</NV_RENAMESCENARIOS>
						<NV_CREATEPACKETS>Create Packets</NV_CREATEPACKETS>
						<NV_REMOVEPACKETS>Remove Packets</NV_REMOVEPACKETS>
						<NV_EXISTINGSCENARIOS>Existing Scenarios</NV_EXISTINGSCENARIOS>
						<NV_REMOVESCENARIO>Remove Scenario</NV_REMOVESCENARIO>
						<NV_RENAMESCENARIO>Rename Scenario</NV_RENAMESCENARIO>
						<NV_REMOVE>Remove</NV_REMOVE>
						<NV_RENAME>Rename</NV_RENAME>
						<NV_ADDPORT>Add or Change Interface</NV_ADDPORT>
						<NV_CHANGEPORT>Remove Interface</NV_CHANGEPORT>
						<NV_CONNECTLINK>Connect Link</NV_CONNECTLINK>
						<NV_DISCONNECTLINK>Disconnect Link</NV_DISCONNECTLINK>
						<NV_PORTNUM>Port [[PORT#]]</NV_PORTNUM>
						<NV_PORTS>Modules</NV_PORTS>
					</LOCKING_TREE>
				</INITIALNET_CONTENT>
				
				<PASSWORD_CONTENT>
					<NV_OPTIONS>Password Options</NV_OPTIONS>
					<NV_DIRECTIONS>Setting a password prevents unauthorized changes to this activity's parameters. When a user is running this activity, the Activity Wizard cannot be accessed unless the correct password is entered.</NV_DIRECTIONS>
					<NV_PASSWORD>Password:</NV_PASSWORD>
					<NV_CONFIRMPASSWORD>Confirm Password:</NV_CONFIRMPASSWORD>
					<NV_ENABLEBTN>Enable Password</NV_ENABLEBTN>
					<NV_DISABLEBTN>Disable Password</NV_DISABLEBTN>
					<NV_MATCH>Password enabled</NV_MATCH>
					<NV_NOMATCH>Password does not match</NV_NOMATCH>
					<NV_DISABLED>Password disabled</NV_DISABLED>
					<NV_PASSWORDEMPTY>Password field is empty</NV_PASSWORDEMPTY>
				</PASSWORD_CONTENT>
                                             </WIZARD>
				
			<RESULTS>
				<NV_TITLE>Activity Results</NV_TITLE>
				<NV_CHECKRESULTS>This shows the results of the activity. A red check next to a component indicates the completion of that component.</NV_CHECKRESULTS>
				<NV_ACTIVITYCOMPLETE>Congratulations! You completed the activity</NV_ACTIVITYCOMPLETE>
				<NV_ACTIVITYINCOMPLETE>You did not complete the activity. Please close this window and try again.</NV_ACTIVITYINCOMPLETE>
				<NV_REQUIREDCOMPONENTS>Required Components</NV_REQUIREDCOMPONENTS>
				<NV_COMPLETEDCOMPONENTS>Completed Components</NV_COMPLETEDCOMPONENTS>
				<NV_COMPONENTTYPES>Component Types</NV_COMPONENTTYPES>
				<NV_IP>IP</NV_IP>
				<NV_ROUTING>Routing</NV_ROUTING>
				<NV_ACL>ACL</NV_ACL>
				<NV_NAT>NAT</NV_NAT>
				<NV_PHYSICAL>Physical</NV_PHYSICAL>
				<NV_SWITCHING>Switching</NV_SWITCHING>
				<NV_OTHERS>Others</NV_OTHERS>
				<NV_CLOSE>Close</NV_CLOSE>
			</RESULTS>
			
			<INSTRUCTIONS>
				<NV_TITLE>Instructions</NV_TITLE>
				<NV_RESET>Reset Activity</NV_RESET>
				<NV_CHECKRESULTS>Check Results</NV_CHECKRESULTS>
			</INSTRUCTIONS>
		</ACTIVITY>
		<WAIT_ICON>
			<NV_MSG>Please Wait...</NV_MSG>
		</WAIT_ICON>
	</GUI>
	<ENGINE>
		<PACKET_INFO_MSG>
			<ROUTER>
				<IN>
					<NV_BROKEN>The router receives the collided frame on Port [[PORT#]]. It drops the frame.</NV_BROKEN>
					<NV_RECEIVE>The [[DEVICE_WORD]] receives the frame on [[PORT_WORD]] [[PORT#]].</NV_RECEIVE>
					<NV_TAGGED_FRAME>The router cannot receive tagged frames. It drops the frame.</NV_TAGGED_FRAME>
					<NV_WAN_ADDRESS>The frame's destination WAN address is the All-destination address.</NV_WAN_ADDRESS>
					<NV_BROADCAST>The frame's destination MAC address is a broadcast address. The router drops it.</NV_BROADCAST>
					<NV_CHECK_MAC>The router checks the frame's destination MAC address against the receiving port's.</NV_CHECK_MAC>
					<NV_MISMATCH_MAC>The destination MAC address does not match the receiving port's. The router drops it.</NV_MISMATCH_MAC>
					<NV_MATCH_MAC>The destination MAC address matches the receiving port's.</NV_MATCH_MAC>
					<NV_NO_IP>The receiving [[PORT_WORD]]'s IP address is not configured. The [[DEVICE_WORD]] drops the packet.</NV_NO_IP>
					<NV_QUEUE_PACKET>The router is processing another packet at this time. It queues the packet for processing at the next available time.</NV_QUEUE_PACKET>
					<NV_DEQUEUE_PACKET>The router takes out the packet from the queue, and processes it.</NV_DEQUEUE_PACKET>
					<NV_CHECK_TTL>The [[DEVICE_WORD]] checks the Time-to-live field in the packet.</NV_CHECK_TTL>
					<NV_TTL_IS_ZERO>The Time-to-live field in the packet is 0. The [[DEVICE_WORD]] drops it.</NV_TTL_IS_ZERO>
					<NV_TTL_IS_NOT_ZERO>The Time-to-live field in the packet is greater than 0.</NV_TTL_IS_NOT_ZERO>
					<NV_LOOK_UP_TABLE>The router looks up the packet's destination IP address in the routing table.</NV_LOOK_UP_TABLE>
					<NV_PORT_HAS_ACL>The receiving port has an inbound traffic access-list with an ID of [[ACL_ID]]. The router checks the packet against the access-list.</NV_PORT_HAS_ACL>
					<NV_ACL_NOT_FOUND>The access-list with an ID of [[ACL_ID]] is not found or empty. The router permits the packet.</NV_ACL_NOT_FOUND>
					<NV_ACL_PERMIT>The packet matches the criteria of the statement: [[STATEMENT]]. The packet is permitted.</NV_ACL_PERMIT>
					<NV_ACL_DENY>The packet matches the criteria of the statement: [[STATEMENT]]. The packet is denied and dropped.</NV_ACL_DENY>
					<NV_IMPLICIT_DENY>The packet does not match the criteria of any statement in the access-list. The packet is denied and dropped by default.</NV_IMPLICIT_DENY>
					<NV_BROADCAST_IP>The packet's destination IP address is a broadcast address. The [[DEVICE_WORD]] drops it.</NV_BROADCAST_IP>
					<NV_MATCH_LOCAL_BROADCAST>The [[DEVICE_WORD]] matches the packet's destination IP address with the broadcast and local addresses.</NV_MATCH_LOCAL_BROADCAST>
					<NV_IP_MATCH>The destination IP address matches [[PORT_WORD]] [[PORT#]]'s IP address.</NV_IP_MATCH>
					<NV_USER_APP>The user application receives the user data.</NV_USER_APP>
					<NV_NO_MATCH_LOCAL_BROADCAST>The destination IP address does not match any local or broadcast addresses.</NV_NO_MATCH_LOCAL_BROADCAST>
					<NV_DE_ENCAP_SEGMENT>The [[DEVICE_WORD]] de-encapsulates the segment data for processing ACL and/or NAT.</NV_DE_ENCAP_SEGMENT>
					<NV_DE_ENCAP_SEGMENT_RECEIVE>The [[DEVICE_WORD]] de-encapsulates the segment data for processing.</NV_DE_ENCAP_SEGMENT_RECEIVE>
					<NV_OUTSIDE_NETWORK>The packet is coming from an outside network. The router looks up its NAT table for necessary translations.</NV_OUTSIDE_NETWORK>
					<NV_NAT_MATCH>The NAT table has a matched entry for this packet. It replaces the inside global address and port with the local ones.</NV_NAT_MATCH>
					<NV_NAT_NO_MATCH>The NAT table does not have a matched entry for this packet. It passes the packet through without translations.</NV_NAT_NO_MATCH>
					<NV_PROCESS_BROADCAST>The frame's destination MAC address is a broadcast address. The router processes it.</NV_PROCESS_BROADCAST>
					<NV_PROCESS_BROADCAST_PACKET>The packet's destination IP address is a broadcast or multicast address. The [[DEVICE_WORD]] processes it.</NV_PROCESS_BROADCAST_PACKET>
					<NV_RECEIVE_RIP_PACKET>The [[DEVICE_WORD]] receives a RIP update packet.</NV_RECEIVE_RIP_PACKET>
					<NV_RIP_NOT_ENABLED>RIP is not enabled on the receiving port. The [[DEVICE_WORD]] drops the update.</NV_RIP_NOT_ENABLED>
					<NV_DIFFERENT_RIP_NETWORK>The RIP update originates from the different network than the receiving port. The [[DEVICE_WORD]] drops the update.</NV_DIFFERENT_RIP_NETWORK>
					<NV_MISMATCH_RIP_VERSION>The RIP update's version does not match this router's RIP version. The [[DEVICE_WORD]] drops the update.</NV_MISMATCH_RIP_VERSION>
					<NV_PROCESS_RIP_NETWORK>The [[DEVICE_WORD]] processes the [[NETWORK]] network update.</NV_PROCESS_RIP_NETWORK>
					<NV_RIP_NETWORK_NOT_EXIST>The [[NETWORK]] network is not in the routing table. The [[DEVICE_WORD]] adds it to the routing table.</NV_RIP_NETWORK_NOT_EXIST>
					<NV_RIP_NETWORK_HAS_LOWER_METRIC>The [[NETWORK]] network is in the routing table but the update has a lower metric than the existing one. The [[DEVICE_WORD]] replaces the old route with the new one.</NV_RIP_NETWORK_HAS_LOWER_METRIC>
					<NV_RIP_NETWORK_HAS_SAME_METRIC>The new route to the [[NETWORK]] network has the same metric as an existing one. The [[DEVICE_WORD]] adds the new route to the routing table.</NV_RIP_NETWORK_HAS_SAME_METRIC>
					<NV_RIP_NETWORK_HAS_LARGER_METRIC>The new route to the [[NETWORK]] network has a larger metric than the existing one. The [[DEVICE_WORD]] ignores the update.</NV_RIP_NETWORK_HAS_LARGER_METRIC>
				</IN>
				<OUT>
					<NV_CLOUD_NO_ROUTE>The cloud does not have a route to the destination. It drops the packet.</NV_CLOUD_NO_ROUTE>
					<NV_ROUTER_NO_ROUTE>The destination IP address is not in the routing table.</NV_ROUTER_NO_ROUTE>
					<NV_NO_GATEWAY>The router does not have a gateway of last resort. It drops the packet.</NV_NO_GATEWAY>
					<NV_HAS_GATEWAY>The router has a gateway of last resort. It sends the packet to the gateway.</NV_HAS_GATEWAY>
					<NV_LOOK_UP_GATEWAY>The router looks up the gateway of last resort in the routing table.</NV_LOOK_UP_GATEWAY>
					<NV_GATEWAY_UNREACHABLE>The router's gateway of last resort is unreachable. The router drops the packet.</NV_GATEWAY_UNREACHABLE>
					<NV_GATEWAY_REACH_VIA_STATIC_ROUTE>The router's gateway of last resort can be reached via [[NEXT_HOP]].</NV_GATEWAY_REACH_VIA_STATIC_ROUTE>
					<NV_GATEWAY_REACH_DIRECTLY>The router's gateway of last resort can be reached through Port [[PORT#]] directly.</NV_GATEWAY_REACH_DIRECTLY>
					<NV_GATEWAY_REACH_VIA_NEXT_HOP>The router's gateway of last resort can be reached through Port [[PORT#]] via [[NEXT_HOP]].</NV_GATEWAY_REACH_VIA_NEXT_HOP>
					<NV_CLOUD_REACH_DIRECTLY>The destination can be reached through [[PORT_WORD]] [[PORT#]] directly.</NV_CLOUD_REACH_DIRECTLY>
					<NV_CLOUD_REACH_VIA>The destination can be reached through [[PORT_WORD]] [[PORT#]] via [[NEXT_HOP]].</NV_CLOUD_REACH_VIA>
					<NV_REACH_VIA_STATIC_ROUTE>The destination IP address is in the routing table. It can be reached via [[NEXT_HOP]].</NV_REACH_VIA_STATIC_ROUTE>
					<NV_REACH_DIRECTLY>The destination IP address is in the routing table. It can be reached through [[PORT_WORD]] [[PORT#]] directly.</NV_REACH_DIRECTLY>
					<NV_REACH_VIA_NEXT_HOP>The destination IP address is in the routing table. It can be reached through [[PORT_WORD]] [[PORT#]] via [[NEXT_HOP]].</NV_REACH_VIA_NEXT_HOP>
					<NV_SAME_PORT>The destination is directly connected to the receiving [[PORT_WORD]]. The [[DEVICE_WORD]] drops the packet.</NV_SAME_PORT>
					<NV_DECREMENT_TTL>The [[DEVICE_WORD]] decrements the Time-to-live field in the packet.</NV_DECREMENT_TTL>
					<NV_SET_WAN_ADDRESS>The [[DEVICE_WORD]] sets the frame's destination WAN address to the All-destination address.</NV_SET_WAN_ADDRESS>
					<NV_LOOK_UP_ARP>The router looks up the Layer 2 destination in its ARP table.</NV_LOOK_UP_ARP>
					<NV_NOT_IN_ARP>The Layer 2 destination is not in ARP table. And an ARP request is sent but no reply is received. The router drops the frame.</NV_NOT_IN_ARP>
					<NV_IN_ARP>The Layer 2 destination is in the ARP table.</NV_IN_ARP>
					<NV_CHANGE_MAC>The router changes the frame's source MAC address to the outgoing port's MAC address, and the destination MAC address to the Layer 2 destination's MAC address.</NV_CHANGE_MAC>
					<NV_SEND_FRAME>The [[DEVICE_WORD]] sends out the frame on [[PORT_WORD]] [[PORT#]].</NV_SEND_FRAME>
					<NV_PORT_HAS_ACL>The outgoing port has an outbound traffic access-list with an ID of [[ACL_ID]]. The router checks the packet against the access-list.</NV_PORT_HAS_ACL>
					<NV_ACL_NOT_FOUND>The access-list with an ID of [[ACL_ID]] is not found or empty. The router permits the packet.</NV_ACL_NOT_FOUND>
					<NV_ACL_PERMIT>The packet matches the criteria of the statement: [[STATEMENT]]. The packet is permitted.</NV_ACL_PERMIT>
					<NV_ACL_DENY>The packet matches the criteria of the statement: [[STATEMENT]]. The packet is denied and dropped.</NV_ACL_DENY>
					<NV_IMPLICIT_DENY>The packet does not match the criteria of any statement in the access-list. The packet is denied and dropped by default.</NV_IMPLICIT_DENY>
					<NV_ENCAP_SEGMENT>The [[DEVICE_WORD]] encapsulates the segment data for sending.</NV_ENCAP_SEGMENT>
					<NV_INSIDE_NETWORK>The packet is going from an inside to an outside network. The router looks up its NAT table for necessary translations.</NV_INSIDE_NETWORK>
					<NV_NAT_NO_MATCH>The NAT table does not have existing translations with inside local address and port. It goes through inside source lists for necessary translations.</NV_NAT_NO_MATCH>
					<NV_NAT_ADD_ENTRY>An inside source entry is created from a list. The new entry is added to the NAT table.</NV_NAT_ADD_ENTRY>
					<NV_NAT_LIST_NO_MATCH>The packet does not match any inside source lists.</NV_NAT_LIST_NO_MATCH>
					<NV_NAT_MATCH>The NAT table has a matched entry for this packet. It replaces the inside local address and port with the global ones.</NV_NAT_MATCH>
					<NV_NAT_NO_TRANS>The NAT table does not have a matched entry for this packet. It passes the packet through without translations.</NV_NAT_NO_TRANS>
					<NV_SET_RIP_VERSION>The [[DEVICE_WORD]] sets the RIP version number to [[VERSION]].</NV_SET_RIP_VERSION>
					<NV_ADD_DIRECT_NETWORKS>The [[DEVICE_WORD]] adds the following directly connected networks to the advertising update:</NV_ADD_DIRECT_NETWORKS>
					<NV_ADD_DST_IP>The [[DEVICE_WORD]] adds destination IP address to the packet.</NV_ADD_DST_IP>
					<NV_ADVERTISE_NETWORK>The [[DEVICE_WORD]] adds the [[NETWORK]] network to be advertised to other routers.</NV_ADVERTISE_NETWORK>
					<NV_SET_FRAME_ADDRESS>The [[DEVICE_WORD]] sets the frame's layer 2 destination address.</NV_SET_FRAME_ADDRESS>
					<NV_RIP_NOT_FORWARD>The [[DEVICE_WORD]] does not forward any updates to other routers.</NV_RIP_NOT_FORWARD>
				</OUT>
				<DEVICE_WORD>
					<NV_CLOUD>cloud</NV_CLOUD>
					<NV_ROUTER>router</NV_ROUTER>
				</DEVICE_WORD>
				<PORT_WORD>
					<NV_BORDER>Border</NV_BORDER>
					<NV_PORT>Port</NV_PORT>
				</PORT_WORD>
			</ROUTER>
			<SWITCH>
				<IN>
					<NV_BROKEN>The [[DEVICEWORD]] receives the collided frame on Port [[FROMPORTNUM]]. It drops the frame.</NV_BROKEN>
					<NV_IS_USER_FRAME>The [[DEVICEWORD]] receives the frame on Port [[FROMPORTNUM]].</NV_IS_USER_FRAME>
					<NV_ACCESS_PORT_TAGGED_FRAME_BRIDGE>The bridge cannot receive tagged frames. It drops the frame.</NV_ACCESS_PORT_TAGGED_FRAME_BRIDGE>
					<NV_ACCESS_PORT_TAGGED_FRAME_SWITCH>Port [[FROMPORTNUM]] is an access port. An access port cannot receive tagged frames. The switch drops the frame.</NV_ACCESS_PORT_TAGGED_FRAME_SWITCH>
					<NV_TRUNK_PORT_TAGGED_FRAME>Port [[FROMPORTNUM]] is a trunk port. A trunk port can only receive tagged frames. The switch drops the frame.</NV_TRUNK_PORT_TAGGED_FRAME>
					<NV_VLAN_TAG_INFORMATION>The switch extracts VLAN tag information from the tagged frame. The frame belongs to VLAN [[VLANNUM]].</NV_VLAN_TAG_INFORMATION>
					<NV_VLAN_NOT_PART_OF_TRUNK_PORT>Trunk port [[FROMPORTNUM]] is not configured to send and receive frames from VLAN [[VLANNUM]]. The switch drops the frame.</NV_VLAN_NOT_PART_OF_TRUNK_PORT>
					<NV_PSECURITY_VIOLATION>A switchport security violation has occured on port(s): [[VIOLATEDPORTS]]</NV_PSECURITY_VIOLATION>
					<NV_CHECK_MAC>The switch's interface Vlan[[VLAN_NUMBER]] is up. It checks the frame's destination MAC address against interface Vlan[[VLAN_NUMBER]]'s.</NV_CHECK_MAC>
					<NV_MAC_NOT_MATCH>The frame's destination does not match interface Vlan[[VLAN_NUMBER]]'s MAC address.</NV_MAC_NOT_MATCH>
					<NV_MAC_MATCH>The frame's destination matches interface Vlan[[VLAN_NUMBER]]'s MAC address.</NV_MAC_MATCH>
					<NV_CHECK_IP>The switch checks the packet's destination IP address with interface Vlan[[VLAN_NUMBER]]'s IP address.</NV_CHECK_IP>
					<NV_IP_NOT_MATCH>The packet's destination IP address does not match interface Vlan[[VLAN_NUMBER]]'s IP address.</NV_IP_NOT_MATCH>
					<NV_IP_MATCH>The packet's destination IP address matches interface Vlan[[VLAN_NUMBER]]'s IP address.</NV_IP_MATCH>					
				</IN>
				<OUT>
					<NV_BROADCAST_FRAME>The frame is a broadcast frame.</NV_BROADCAST_FRAME>
					<NV_BROADCAST_FORWARD_BRIDGE>The bridge forwards the frame out to the other port.</NV_BROADCAST_FORWARD_BRIDGE>
					<NV_BROADCAST_FORWARD_SWITCH>The switch floods the frame out to all ports in VLAN [[VLANNUM]] except the receiving port.</NV_BROADCAST_FORWARD_SWITCH>
					<NV_UNICAST_FRAME>The frame is a unicast frame. The [[DEVICEWORD]] looks up the frame's destination MAC address in the MAC table.</NV_UNICAST_FRAME>
					<NV_UNICAST_DST_NOT_IN_MAC_TABLE>The destination MAC address is not in the MAC table.</NV_UNICAST_DST_NOT_IN_MAC_TABLE>
					<NV_NOT_FOUND_BRIDGE_FORWARD>The bridge forwards the frame out to the other port.</NV_NOT_FOUND_BRIDGE_FORWARD>
					<NV_NOT_FOUND_SWITCH_FORWARD>The switch floods the frame out to all ports in VLAN [[VLANNUM]] except the receiving port.</NV_NOT_FOUND_SWITCH_FORWARD>
					<NV_MAC_FOUND>The destination MAC address is in the MAC table, and it can be reached through Port [[PORTNUM]]</NV_MAC_FOUND>
					<NV_OUT_PORT_SAME_AS_IN>The outgoing port is the same as the receiving port. The [[DEVICEWORD]] drops the frame.</NV_OUT_PORT_SAME_AS_IN>
					<NV_SWITCH_TAG_FRAME>The switch tags the frame with VLAN information for going out on Trunk Port(s): [[OUTPORTLIST]].</NV_SWITCH_TAG_FRAME>
					<NV_SEND_FRAME>The [[DEVICEWORD]] sends out the frame on Port(s): [[OUTPORTLIST]]</NV_SEND_FRAME>
					<NV_NON_FUNC_PORT_BRIDGE>The bridge's other port is not functional. The frame is not forwarded.</NV_NON_FUNC_PORT_BRIDGE>
					<NV_NON_FUNC_PORT_SWITCH>The switch does not have any other functional ports to send. The frame is not forwarded.</NV_NON_FUNC_PORT_SWITCH>
					<NV_PSECURITY_VIOLATION>A switchport security violation has occured on port(s): [[VIOLATEDPORTS]]</NV_PSECURITY_VIOLATION>
					<NV_NO_FUNC_VLAN_INT>The switch does not have a functional Vlan interface. It drops the packet.</NV_NO_FUNC_VLAN_INT>
					<NV_NO_IP_ADDRESS>The switch's interface Vlan[[VLAN_NUMBER]] does not have an IP address. It drops the packet.</NV_NO_IP_ADDRESS>
					<NV_ADD_IP_TO_SOURCE>The switch adds interface Vlan[[VLAN_NUMBER]]'s IP address as the source IP address.</NV_ADD_IP_TO_SOURCE>
					<NV_VLAN_INT_DOWN>The switch's interface Vlan[[VLAN_NUMBER]] is down. It drops the frame.</NV_VLAN_INT_DOWN>
					<NV_ADD_MAC_TO_SOURCE>The switch adds its interface Vlan[[VLAN_NUMBER]]'s MAC address as the source MAC address.</NV_ADD_MAC_TO_SOURCE>
				</OUT>
				<DEVICE_WORD>
					<NV_BRIDGE>bridge</NV_BRIDGE>
					<NV_SWITCH>switch</NV_SWITCH>
				</DEVICE_WORD>
			</SWITCH>
			<REPEATER>
				<IN>
					<NV_FRAME_RECEIVED>The repeater receives the frame on Port [[FROMPORTNUM]].</NV_FRAME_RECEIVED>
				</IN>
				<OUT>
					<NV_SEND_FRAME>The repeater sends out the frame on Port [[PORTNUM]].</NV_SEND_FRAME>
					<NV_NO_FUNC_PORTS>Port [[PORTNUM]] is not functional. The frame is not forwarded.</NV_NO_FUNC_PORTS>
				</OUT>
			</REPEATER>
			<HUB>
				<IN>
					<NV_FRAME_RECEIVED>The hub receives the frame on Port [[FROMPORTNUM]].</NV_FRAME_RECEIVED>
				</IN>
				<OUT>
					<NV_SEND_FRAME>The hub sends out the frame on Port(s): [[OUTPORTLIST]].</NV_SEND_FRAME>
					<NV_NO_FUNC_PORTS>The hub does not have any other functional ports to send. The frame is not forwarded.</NV_NO_FUNC_PORTS>
				</OUT>
			</HUB>
			<ACCESS_POINT>
				<IN>
					<NV_FRAME_RECEIVED>The access point receives the frame on Port [[FROMPORTNUM]].</NV_FRAME_RECEIVED>
				</IN>
				<OUT>
					<NV_SEND_FRAME>The access point sends out the frame on Port(s): [[OUTPORTLIST]].</NV_SEND_FRAME>
					<NV_NO_FUNC_PORTS>The access point does not have any other functional ports to send. The frame is not forwarded.</NV_NO_FUNC_PORTS>
				</OUT>
			</ACCESS_POINT>
			<PC>
				<IN>
					<NV_BROKEN_FRAME>The [[DEVICE_TYPE]] receives the collided frame. It drops the frame.</NV_BROKEN_FRAME>
					<NV_FRAME_RECEIVED>The [[DEVICE_TYPE]] receives the frame.</NV_FRAME_RECEIVED>
					<NV_IS_WAN_PORT>The frame's destination WAN address is the All-destination address.</NV_IS_WAN_PORT>
					<NV_BROADCAST>The destination MAC address is the broadcast address. The [[DEVICE_TYPE]] processes the frame.</NV_BROADCAST>
					<NV_CHECK_MAC>The [[DEVICE_TYPE]] checks the frame's destination MAC address against its own.</NV_CHECK_MAC>
					<NV_MAC_NOT_MATCH>The destination MAC address does not match the [[DEVICE_TYPE]]'s MAC address. The [[DEVICE_TYPE]] drops the frame.</NV_MAC_NOT_MATCH>
					<NV_MAC_MATCHES>The destination MAC address matches the [[DEVICE_TYPE]]'s MAC address.</NV_MAC_MATCHES>
					<NV_NOT_FUNC>The [[DEVICE_TYPE]]'s IP address is not configured. The [[DEVICE_TYPE]] drops the packet.</NV_NOT_FUNC>
					<NV_CHECK_IP>The [[DEVICE_TYPE]] checks the packet's destination IP address against its own.</NV_CHECK_IP>
					<NV_IP_NOT_MATCH>The destination IP address does not match the [[DEVICE_TYPE]]'s IP address. The [[DEVICE_TYPE]] drops the packet.</NV_IP_NOT_MATCH>
					<NV_IP_MATCH>The destination IP address matches the [[DEVICE_TYPE]]'s IP address.</NV_IP_MATCH>
					<NV_USER_APP>The user application receives the user data.</NV_USER_APP>
					<NV_DE_ENCAP_SEGMENT>The [[DEVICE_TYPE]] de-encapsulates the segment data for processing.</NV_DE_ENCAP_SEGMENT>
				</IN>
				<OUT>
					<NV_SEND_FRAME_APP>The user application sends out the user data.</NV_SEND_FRAME_APP>
					<NV_NO_FUNC_PORT>The [[DEVICE_TYPE]] does not have a port. It drops the packet.</NV_NO_FUNC_PORT>
					<NV_NO_IP_ADDRESS>The [[DEVICE_TYPE]] does not have an IP address. It drops the packet.</NV_NO_IP_ADDRESS>
					<NV_ADD_IP_TO_SOURCE>The [[DEVICE_TYPE]] adds its IP address as the source IP address.</NV_ADD_IP_TO_SOURCE>
					<NV_PORT_DOWN>The [[DEVICE_TYPE]]'s port is down. It drops the frame.</NV_PORT_DOWN>
					<NV_IS_WAN_PORT>The [[DEVICE_TYPE]] sets the frame's destination WAN address to the All-destination address.</NV_IS_WAN_PORT>
					<NV_ADD_MAC_TO_SOURCE>The [[DEVICE_TYPE]] adds the entry's MAC address as the source MAC address.</NV_ADD_MAC_TO_SOURCE>
					<NV_DST_IN_LAN>The destination is in the same LAN as this [[DEVICE_TYPE]]. The [[DEVICE_TYPE]] sends the frame to it directly.</NV_DST_IN_LAN>
					<NV_DST_NOT_IN_LAN>The destination is not in the same LAN as this [[DEVICE_TYPE]]. The [[DEVICE_TYPE]] sends the frame to the default gateway.</NV_DST_NOT_IN_LAN>
					<NV_DST_UNREACHABLE>The destination is not in the same LAN as this [[DEVICE_TYPE]], and this [[DEVICE_TYPE]] does not have a default gateway. The [[DEVICE_TYPE]] drops the frame.</NV_DST_UNREACHABLE>
					<NV_ARP_LOOKUP>The [[DEVICE_TYPE]] looks up the MAC address of the Layer 2 destination in its ARP table.</NV_ARP_LOOKUP>
					<NV_ARP_NOT_FOUND>The Layer 2 destination is not in the ARP table. And an ARP request is sent but no reply is received. The [[DEVICE_TYPE]] drops the frame.</NV_ARP_NOT_FOUND>
					<NV_ARP_FOUND>The Layer 2 destination is in the ARP table. The [[DEVICE_TYPE]] adds its MAC address as the destination MAC address.</NV_ARP_FOUND>
					<NV_SEND_FRAME>The [[DEVICE_TYPE]] sends out the frame.</NV_SEND_FRAME>
					<NV_ENCAP_SEGMENT>The [[DEVICE_TYPE]] encapsulates the segment data for sending.</NV_ENCAP_SEGMENT>
				</OUT>
				<DEVICE_TYPE>
					<NV_PC>PC</NV_PC>
					<NV_SERVER>server</NV_SERVER>
					<NV_PRINTER>printer</NV_PRINTER>
					<NV_ROUTER>router</NV_ROUTER>
					<NV_SWITCH>switch</NV_SWITCH>
				</DEVICE_TYPE>
			</PC>
			<SWITCH_PORT>
				<NV_QUEUE_FRAME>Port [[PORT#]] is sending another frame at this time. The switch queues the frame for sending at the next available time.</NV_QUEUE_FRAME>
				<NV_DEQUEUE_FRAME>The switch takes out the frame from the queue, and sends it out on Port [[PORT#]].</NV_DEQUEUE_FRAME>
			</SWITCH_PORT>
			<CLOUD_BORDER>
				<NV_QUEUE_FRAME>Border [[PORT#]] is sending another frame at this time. The cloud queues the frame for sending at the next available time.</NV_QUEUE_FRAME>
				<NV_DEQUEUE_FRAME>The cloud takes out the frame from the queue, and sends it out on Border [[PORT#]].</NV_DEQUEUE_FRAME>
				<NV_FRAME_ON_TRANSIT>The frame is on transit in the cloud.</NV_FRAME_ON_TRANSIT>
				<NV_FRAME_DONE_TRANSIT>The frame reaches the border of the cloud after [[DELAY]] units of time on transit. The cloud sends the frame out on Border [[PORT#]].</NV_FRAME_DONE_TRANSIT>
			</CLOUD_BORDER>
			<FRAME_INSTANCE>
				<NV_MILLISEC> ms</NV_MILLISEC>
				<NV_AT_DEVICE>At Device: </NV_AT_DEVICE>
				<NV_SOURCE>Source: </NV_SOURCE>
				<NV_DESTINATION>Destination: </NV_DESTINATION>
				<NV_COLLIDED>The following frames collided with each other:</NV_COLLIDED>
				<NV_TRANSMISSION_TIME>TX time: </NV_TRANSMISSION_TIME>
				<NV_LAYER>Layer [[LAYER#]]</NV_LAYER>
				<NV_USER_DATA>&lt;User data&gt;</NV_USER_DATA>
				<NV_ENCAPSULATE>Encapsulate</NV_ENCAPSULATE>
				<NV_DE_ENCAPSULATE>De-encapsulate</NV_DE_ENCAPSULATE>
				<NV_PROCESS>Process</NV_PROCESS>
				<NV_QUEUE>Queue</NV_QUEUE>
				<NV_DROP>Drop</NV_DROP>
				<NV_FORWARD>Forward</NV_FORWARD>
				<NV_SEND>Send</NV_SEND>
				<NV_RECEIVE>Receive</NV_RECEIVE>
				<NV_TTL_EQUAL>TTL = </NV_TTL_EQUAL>
				<NV_PROTOCOL_EQUAL>Protocol = </NV_PROTOCOL_EQUAL>
				<NV_SEQUENCE_NUMBER_EQUAL>Sequence # = </NV_SEQUENCE_NUMBER_EQUAL>
				<NV_PORTS_EQUAL>Ports = </NV_PORTS_EQUAL>
				<NV_SRC>Source:</NV_SRC>
				<NV_DST>Dest:</NV_DST>
				<NV_TTL>TTL:</NV_TTL>
				<NV_PROTOCOL>Protocol:</NV_PROTOCOL>
				<NV_SRC_PORT>Source Port:</NV_SRC_PORT>
				<NV_DST_PORT>Dest Port:</NV_DST_PORT>
				<NV_SEQUENCE_NUMBER>Sequence #:</NV_SEQUENCE_NUMBER>
			</FRAME_INSTANCE>
			<TIMELINE_PACKET_INFO>
				<NV_BROADCAST>Broadcast</NV_BROADCAST>
				<NV_UNKNOWN>Unknown</NV_UNKNOWN>
			</TIMELINE_PACKET_INFO>
		</PACKET_INFO_MSG>
		<LINK>
			<NV_TWO_CLOUDS>A connection cannot be made between two clouds. Please select another device.</NV_TWO_CLOUDS>
			<NV_WRONG_TYPE>A [[LINK_TYPE]] link cannot be connected to a [[PORT_TYPE]] port. Please select another port.</NV_WRONG_TYPE>
			<NV_TWO_ACCESS_POINTS>A connection cannot be made between two access points using wireless. Please select another device.</NV_TWO_ACCESS_POINTS>
			<NV_TWO_PCS_WIRELESS>A connection cannot be made between two hosts using wireless. Please select another port.</NV_TWO_PCS_WIRELESS>
			<NV_TWO_PCS_PHONE>A connection cannot be made between two hosts using phone line. Please select another device.</NV_TWO_PCS_PHONE>
			<NV_CANNOT_CONNECT>A connection cannot be made between a [[PORT1_TYPE]] port and a [[PORT2_TYPE]] port.</NV_CANNOT_CONNECT>
		</LINK>
	</ENGINE>
</LANGUAGE>
