<LANGUAGE FOR="Packet Tracer 3.2 Help Files">
	<GUI_LANGUAGE_FILE>default.ptl</GUI_LANGUAGE_FILE>
	<TEMP>
		<NV_0></NV_0>
	</TEMP>
	<SIMULATION_PANEL>
		<NV_0>Scenario Description</NV_0>
		<NV_1>Scenario Select</NV_1>
		<NV_2>Add Packet</NV_2>
		<NV_3>Timeline</NV_3>
		<NV_4>Time Frame Indicator</NV_4>
		<NV_5>Timeline Navigation</NV_5>
		<NV_6>Simulation Controls</NV_6>
		<NV_7>Add/Delete Scenario</NV_7>
		<NV_8>Delete Packet</NV_8>
		<NV_9>Packet Color Picker</NV_9>
		<NV_10>Existing Packets</NV_10>
		<NV_11>Packets Scrollbar</NV_11>
		<NV_12>Fast Rewind</NV_12>
		<NV_13>Current Frame</NV_13>
		<NV_14>Fast Fwd</NV_14>
		<NV_15>Back Step</NV_15>
		<NV_16>Play/Pause</NV_16>
		<NV_17>Speed Slider</NV_17>
		<NV_18>Fwd Step</NV_18>
	</SIMULATION_PANEL>
	<FLOW_ROUTER>
		<NV_START>Router receives a frame</NV_START>
		<NV_END>End</NV_END>
		<NV_YES>Yes</NV_YES>
		<NV_NO>No</NV_NO>
		<NV_D4>Is the receiving port a WAN port?</NV_D4>
		<NV_D5>Is the frame a broadcast frame?</NV_D5>
		<NV_D6>Does destination MAC address match the receiving port's?</NV_D6>
		<NV_D7>IS packet's TTL > 0?</NV_D7>
		<NV_D8>Does receiving port have an inbound ACL?</NV_D8>
		<NV_D9>Does packet pass the inbound ACL?</NV_D9>
		<NV_D10>Is the receiving port a NAT outside port?</NV_D10>
		<NV_D11>Does NAT table have matching entry?</NV_D11>
		<NV_D12>Does routing table have matching entry?</NV_D12>
		<NV_D13>Does router have a gateway of last resort?</NV_D13>
		<NV_D14>Is the network in the entry directly connected?</NV_D14>
		<NV_D15>Is the receiving port a NAT inside port and the outgoing port a NAT outside port?</NV_D15>
		<NV_D16>Does NAT table have matching entry?</NV_D16>
		<NV_D17>Does packet match any inside NAT source list?</NV_D17>
		<NV_D18>Does outgoing port have an outbound ACL?</NV_D18>
		<NV_D19>Does packet pass the outbound ACL?</NV_D19>
		<NV_D20>Is the outgoing port a WAN port?</NV_D20>
		<NV_D21></NV_D21>
		<NV_D22></NV_D22>
		<NV_D23></NV_D23>
		<NV_D24></NV_D24>
		<NV_D25></NV_D25>
		<NV_D26></NV_D26>
		<NV_D27></NV_D27>
		<NV_D28></NV_D28>
		<NV_D29></NV_D29>
		<NV_A30>Drop the frame.</NV_A30>
		<NV_A31>Look up packet's destination IP in the NAT table as global address.</NV_A31>
		<NV_A32>Look up packet's destination network in the routing table.</NV_A32>
		<NV_A33>Translate destination IP and port numbers to the entry's.</NV_A33>
		<NV_A34>Mark the packet's destination as the next hop level 2 destination.</NV_A34>
		<NV_A35>Mark the layer 3 next hop as the next hop level 2 destination.</NV_A35>
		<NV_A36>Mark the gateway of last resort as the next hop level 2 destination.</NV_A36>
		<NV_A37>Look up packet's source IP in the NAT table as local address.</NV_A37>
		<NV_A38>Add new NAT entry to NAT table.</NV_A38>
		<NV_A39>Translate source IP and port numbers to the entry's.</NV_A39>
		<NV_A40>Set the frame's destination address to the all-destination address.</NV_A40>
		<NV_A41>Set the frame's destination address to the MAC address of the next hop level 2 destination.</NV_A41>
		<NV_A42>Set the frame's source address to the MAC address of the outgoing port.</NV_A42>
		<NV_A43>Forward the packet out the outgoing port.</NV_A43>
		<NV_A44></NV_A44>
		<NV_A45></NV_A45>
		<NV_A46></NV_A46>
		<NV_A47></NV_A47>
		<NV_A48></NV_A48>
	</FLOW_ROUTER>
	<FLOW_SWITCH>
		<NV_START>Switch receives a frame.</NV_START>
		<NV_END>End</NV_END>
		<NV_YES>Yes</NV_YES>
		<NV_NO>No</NV_NO>
		<NV_D4>Is the receiving port an access port?</NV_D4>
		<NV_D5>Is the frame a tagged frame?</NV_D5>
		<NV_D6>Is the frame a tagged frame?</NV_D6>
		<NV_D7>Does the frame pass the receiving port's port-security?</NV_D7>
		<NV_D8>Is the receiving VLAN a member of the reciving trunk port?</NV_D8>
		<NV_D9>Is the frame's destination MAC address the broadcast address?</NV_D9>
		<NV_D10>Is a matching entry found in the MAC table?</NV_D10>
		<NV_D11>Is the outgoing port the same as the receiving port?</NV_D11>
		<NV_D12>Does the frame pass the outgoing port(s) port-security?</NV_D12>
		<NV_D13></NV_D13>
		<NV_D14></NV_D14>
		<NV_D15></NV_D15>
		<NV_D16></NV_D16>
		<NV_D17></NV_D17>
		<NV_D18></NV_D18>
		<NV_D19></NV_D19>
		<NV_D20></NV_D20>
		<NV_D21></NV_D21>
		<NV_D22></NV_D22>
		<NV_D23></NV_D23>
		<NV_D24></NV_D24>
		<NV_D25></NV_D25>
		<NV_D26></NV_D26>
		<NV_D27></NV_D27>
		<NV_D28></NV_D28>
		<NV_D29></NV_D29>
		<NV_A30>Mark the receiving port's access VLAN as the receiving VLAN.</NV_A30>
		<NV_A31>Extract VLAN number from tag and mark it as the receiving VLAN.</NV_A31>
		<NV_A32>Look up the destination MAC address in the receiving VLAN's MAC table.</NV_A32>
		<NV_A33>Send frame out to all ports in the receiving VLAN except the receiving one.</NV_A33>
		<NV_A34>Send frame out the outgoing port.</NV_A34>
		<NV_A35>Drop the frame.</NV_A35>
		<NV_A36></NV_A36>
		<NV_A37></NV_A37>
		<NV_A38></NV_A38>
		<NV_A39></NV_A39>
		<NV_A40></NV_A40>
		<NV_A41></NV_A41>
		<NV_A42></NV_A42>
		<NV_A43></NV_A43>
		<NV_A44></NV_A44>
		<NV_A45></NV_A45>
		<NV_A46></NV_A46>
		<NV_A47></NV_A47>
		<NV_A48></NV_A48>
	</FLOW_SWITCH>
	<FLOW_PC_SENDFRAME>
		<NV_START>A frame is to be sent from the PC.</NV_START>
		<NV_END>End</NV_END>
		<NV_YES>Yes</NV_YES>
		<NV_NO>No</NV_NO>
		<NV_D4>Is the PC port a WAN port?</NV_D4>
		<NV_D5>Did user specify a destination MAC address?</NV_D5>
		<NV_D6>Is the destination in the same network as the PC?</NV_D6>
		<NV_D7>Does this PC have a default gateway?</NV_D7>
		<NV_D8>Does ARP table have matching entry?</NV_D8>
		<NV_D9></NV_D9>
		<NV_D10></NV_D10>
		<NV_D11></NV_D11>
		<NV_D12></NV_D12>
		<NV_D13></NV_D13>
		<NV_D14></NV_D14>
		<NV_D15></NV_D15>
		<NV_D16></NV_D16>
		<NV_D17></NV_D17>
		<NV_D18></NV_D18>
		<NV_D19></NV_D19>
		<NV_D20></NV_D20>
		<NV_D21></NV_D21>
		<NV_D22></NV_D22>
		<NV_D23></NV_D23>
		<NV_D24></NV_D24>
		<NV_D25></NV_D25>
		<NV_D26></NV_D26>
		<NV_D27></NV_D27>
		<NV_D28></NV_D28>
		<NV_D29></NV_D29>
		<NV_A30>Set the destination WAN address to the All-destination address.</NV_A30>
		<NV_A31>Look up MAC address of destination in ARP table.</NV_A31>
		<NV_A32>Look up MAC address of default gateway in ARP table.</NV_A32>
		<NV_A33>Drop the frame.</NV_A33>
		<NV_A34>Set the frame's destination MAC to the matching entry's.</NV_A34>
		<NV_A35>Send the frame.</NV_A35>
		<NV_A36></NV_A36>
		<NV_A37></NV_A37>
		<NV_A38></NV_A38>
		<NV_A39></NV_A39>
		<NV_A40></NV_A40>
		<NV_A41></NV_A41>
		<NV_A42></NV_A42>
		<NV_A43></NV_A43>
		<NV_A44></NV_A44>
		<NV_A45></NV_A45>
		<NV_A46></NV_A46>
		<NV_A47></NV_A47>
		<NV_A48></NV_A48>
	</FLOW_PC_SENDFRAME>
	<FLOW_PC>
		<NV_START>PC receives a frame.</NV_START>
		<NV_END>End</NV_END>
		<NV_YES>Yes</NV_YES>
		<NV_NO>No</NV_NO>
		<NV_D4>Is the port a WAN port?</NV_D4>
		<NV_D5>Is the frame's destination MAC address the broadcast address?</NV_D5>
		<NV_D6>Does the frame's destination MAC address match the port's?</NV_D6>
		<NV_D7>Does the packet's destination IP address match the PC's?</NV_D7>
		<NV_D8></NV_D8>
		<NV_D9></NV_D9>
		<NV_D10></NV_D10>
		<NV_D11></NV_D11>
		<NV_D12></NV_D12>
		<NV_D13></NV_D13>
		<NV_D14></NV_D14>
		<NV_D15></NV_D15>
		<NV_D16></NV_D16>
		<NV_D17></NV_D17>
		<NV_D18></NV_D18>
		<NV_D19></NV_D19>
		<NV_D20></NV_D20>
		<NV_D21></NV_D21>
		<NV_D22></NV_D22>
		<NV_D23></NV_D23>
		<NV_D24></NV_D24>
		<NV_D25></NV_D25>
		<NV_D26></NV_D26>
		<NV_D27></NV_D27>
		<NV_D28></NV_D28>
		<NV_D29></NV_D29>
		<NV_A30>Drop the packet.</NV_A30>
		<NV_A31>Process the packet.</NV_A31>
		<NV_A32></NV_A32>
		<NV_A33></NV_A33>
		<NV_A34></NV_A34>
		<NV_A35></NV_A35>
		<NV_A36></NV_A36>
		<NV_A37></NV_A37>
		<NV_A38></NV_A38>
		<NV_A39></NV_A39>
		<NV_A40></NV_A40>
		<NV_A41></NV_A41>
		<NV_A42></NV_A42>
		<NV_A43></NV_A43>
		<NV_A44></NV_A44>
		<NV_A45></NV_A45>
		<NV_A46></NV_A46>
		<NV_A47></NV_A47>
		<NV_A48></NV_A48>
	</FLOW_PC>
	<FLOW_HUB>
		<NV_START>Hub receives a frame.</NV_START>
		<NV_END>End</NV_END>
		<NV_A2>Forward the frame out all ports except the incoming port.</NV_A2>
	</FLOW_HUB>
	<FLOW_REPEATER>
		<NV_START>Repeater receives a frame.</NV_START>
		<NV_END>End</NV_END>
		<NV_A2>Forward the frame out the other port.</NV_A2>
	</FLOW_REPEATER>
	<FLOW_ACESSPOINT>
		<NV_START>Access Point receives a packet on its wireless or ethernet port.</NV_START>
		<NV_END>End</NV_END>
		<NV_A2>Forward the packet out the other port.</NV_A2>
	</FLOW_ACESSPOINT>
	<ACTIVITY>
		<NV_INSTURCT_DEMO>This activity tests your ability to make manual connections between devices. Note that Simple Mode is turned off. First, create a router (Router0) and a PC (PC0). Then, connect them over a fast ethernet crossover connection, using  the first port of each device.
		</NV_INSTRUCT_DEMO>
	</ACTIVITY>
</LANGUAGE>
