Lab 7.2.2 Configuring RIP

Objective

- Setup an IP addressing scheme using class B networks.

- Configure the RIP dynamic routing protocol on routers.

Step 1

a) Disable Simple mode and Auto DHCP mode.

b) Enable Console mode and Auto DHCP mode.

c) Open a terminal session to the routers and from the global configuration mode, configure the hostname as shown in the chart.

Step 2

a) From the global configuration mode, enter the following:

GAD(config)#router rip

GAD(config-router)#network 172.16.0.0

GAD(config-router)#network 172.17.0.0

GAD(config-router)#exit

GAD(config)#exit

Step 3

GAD#copy running-config startup-config

Step 4

a) From the global configuration mode, enter the following:

BHM(config)#router rip

BHM(config-router)#network 172.17.0.0

BHM(config-router)#network 172.18.0.0

BHM(config-router)#exit

BHM(config)#exit

Step 5

BHM#copy running-config startup-config

Step 6

a) Configure the hosts with the proper IP address, subnet mask and default gateway.

Step 7

a) Enter into Simulation Mode.

b) Create a packet from one host to the other and view the packet info in detail for each step.

Step 8

a) While in Simulation Mode, open the router terminal windows and display their routing tables.

b) What are the entries in the GAD routing table?

__________________________________________________________________________

c) What are the entries in the BHM routing table?

__________________________________________________________________________