<PACKETTRACER><VERSION>3.2</VERSION><NETWORK><DEVICES><DEVICE><NAME>PC 0</NAME><POWER>true</POWER><X>-145</X><Y>-82</Y><PORTS><PORT><POWER>true</POWER><PORTTYPE>Copper Fast Ethernet</PORTTYPE><BANDWIDTH>100000</BANDWIDTH><FULLDUPLEX>false</FULLDUPLEX><AUTONEGOTIATE>true</AUTONEGOTIATE><CLOCKENABLED>false</CLOCKENABLED><OWNERDEVICE>0</OWNERDEVICE><LINKNUMBER>0</LINKNUMBER><MAC>0000.0cb4.eb26</MAC><SUBNETMASK /><IPADDRESS /><PORTNUMBER>0</PORTNUMBER></PORT><RS232><OWNERDEVICE>0</OWNERDEVICE><LINKNUMBER /><PORTTYPE>RS 232</PORTTYPE><BITSPERSECOND>9600</BITSPERSECOND><DATABITS>8</DATABITS><PARITY>2</PARITY><STOPBITS>1</STOPBITS><FLOWCONTROl>0</FLOWCONTROl></RS232></PORTS><TYPE>o_pc</TYPE><GATEWAY /><DESCRIPTION>PC 0
IP Address: 192.168.1.1
Subnet Mask: 255.255.255.0</DESCRIPTION></DEVICE><DEVICE><NAME>PC 1</NAME><POWER>true</POWER><X>119</X><Y>-79</Y><PORTS><PORT><POWER>true</POWER><PORTTYPE>Copper Fast Ethernet</PORTTYPE><BANDWIDTH>100000</BANDWIDTH><FULLDUPLEX>false</FULLDUPLEX><AUTONEGOTIATE>true</AUTONEGOTIATE><CLOCKENABLED>false</CLOCKENABLED><OWNERDEVICE>1</OWNERDEVICE><LINKNUMBER>1</LINKNUMBER><MAC>000d.bd92.bc5b</MAC><SUBNETMASK /><IPADDRESS /><PORTNUMBER>0</PORTNUMBER></PORT><RS232><OWNERDEVICE>1</OWNERDEVICE><LINKNUMBER /><PORTTYPE>RS 232</PORTTYPE><BITSPERSECOND>9600</BITSPERSECOND><DATABITS>8</DATABITS><PARITY>2</PARITY><STOPBITS>1</STOPBITS><FLOWCONTROl>0</FLOWCONTROl></RS232></PORTS><TYPE>o_pc</TYPE><GATEWAY /><DESCRIPTION>PC 1
IP Address: 192.168.1.2
Subnet Mask: 255.255.255.0</DESCRIPTION></DEVICE><DEVICE><NAME>Hub 0</NAME><POWER>true</POWER><X>-16</X><Y>-35</Y><PORTS><PORT><POWER>true</POWER><PORTTYPE>Copper Fast Ethernet</PORTTYPE><BANDWIDTH>100000</BANDWIDTH><FULLDUPLEX>false</FULLDUPLEX><AUTONEGOTIATE>true</AUTONEGOTIATE><CLOCKENABLED>false</CLOCKENABLED><OWNERDEVICE>2</OWNERDEVICE><LINKNUMBER>0</LINKNUMBER><MAC /><SUBNETMASK /><IPADDRESS /><PORTNUMBER>0</PORTNUMBER></PORT><PORT><POWER>true</POWER><PORTTYPE>Copper Fast Ethernet</PORTTYPE><BANDWIDTH>100000</BANDWIDTH><FULLDUPLEX>false</FULLDUPLEX><AUTONEGOTIATE>true</AUTONEGOTIATE><CLOCKENABLED>false</CLOCKENABLED><OWNERDEVICE>2</OWNERDEVICE><LINKNUMBER>1</LINKNUMBER><MAC /><SUBNETMASK /><IPADDRESS /><PORTNUMBER>1</PORTNUMBER></PORT><PORT><POWER>true</POWER><PORTTYPE>Copper Fast Ethernet</PORTTYPE><BANDWIDTH>100000</BANDWIDTH><FULLDUPLEX>true</FULLDUPLEX><AUTONEGOTIATE>true</AUTONEGOTIATE><CLOCKENABLED>false</CLOCKENABLED><OWNERDEVICE>2</OWNERDEVICE><LINKNUMBER /><MAC /><SUBNETMASK /><IPADDRESS /><PORTNUMBER>2</PORTNUMBER></PORT><PORT><POWER>true</POWER><PORTTYPE>Copper Fast Ethernet</PORTTYPE><BANDWIDTH>100000</BANDWIDTH><FULLDUPLEX>true</FULLDUPLEX><AUTONEGOTIATE>true</AUTONEGOTIATE><CLOCKENABLED>false</CLOCKENABLED><OWNERDEVICE>2</OWNERDEVICE><LINKNUMBER /><MAC /><SUBNETMASK /><IPADDRESS /><PORTNUMBER>3</PORTNUMBER></PORT><PORT><POWER>true</POWER><PORTTYPE>Copper Fast Ethernet</PORTTYPE><BANDWIDTH>100000</BANDWIDTH><FULLDUPLEX>true</FULLDUPLEX><AUTONEGOTIATE>true</AUTONEGOTIATE><CLOCKENABLED>false</CLOCKENABLED><OWNERDEVICE>2</OWNERDEVICE><LINKNUMBER /><MAC /><SUBNETMASK /><IPADDRESS /><PORTNUMBER>4</PORTNUMBER></PORT><PORT><POWER>true</POWER><PORTTYPE>Copper Fast Ethernet</PORTTYPE><BANDWIDTH>100000</BANDWIDTH><FULLDUPLEX>true</FULLDUPLEX><AUTONEGOTIATE>true</AUTONEGOTIATE><CLOCKENABLED>false</CLOCKENABLED><OWNERDEVICE>2</OWNERDEVICE><LINKNUMBER /><MAC /><SUBNETMASK /><IPADDRESS /><PORTNUMBER>5</PORTNUMBER></PORT></PORTS><TYPE>o_hub</TYPE><DESCRIPTION>A Hub is a multi-port repeater. It can regenerate signals but does not filter traffic.</DESCRIPTION></DEVICE></DEVICES><LINKS><LINK><LINKTYPE>Copper Straight-through</LINKTYPE><PORT1><DEVICE>0</DEVICE><PORT>0</PORT></PORT1><PORT2><DEVICE>2</DEVICE><PORT>0</PORT></PORT2><DCEPORT><DEVICE /><PORT /></DCEPORT></LINK><LINK><LINKTYPE>Copper Straight-through</LINKTYPE><PORT1><DEVICE>2</DEVICE><PORT>1</PORT></PORT1><PORT2><DEVICE>1</DEVICE><PORT>0</PORT></PORT2><DCEPORT><DEVICE /><PORT /></DCEPORT></LINK></LINKS><ROUTERS>0</ROUTERS><CLOUDS>0</CLOUDS><SWITCHES>0</SWITCHES><BRIDGES>0</BRIDGES><HUBS>1</HUBS><REPEATERS>0</REPEATERS><ACCESSPOINTS>0</ACCESSPOINTS><PCS>4</PCS><DESCRIPTION>This is a simple hub-based network. Straight through-cables are used to connect the PCs to the hub.</DESCRIPTION><SERVERS>0</SERVERS><PRINTERS>0</PRINTERS><PASS></PASS></NETWORK><SCENARIOSET><CURRENTSCENARIO>0</CURRENTSCENARIO><SCENARIONUMBER>1</SCENARIONUMBER><SCENARIOS><SCENARIO1><NAME>Scenario 0</NAME><KEYFRAMES><KEYFRAME0><TIME>1</TIME><FRAME><DSTMAC>000d.bd92.bc5b</DSTMAC><PACKET><DSTIP>192.168.1.2</DSTIP><TTL>32</TTL><PROTOCOL>0</PROTOCOL><SEGMENT><SRCPORT>272</SRCPORT><DSTPORT>272</DSTPORT></SEGMENT></PACKET><SRCDEVICE>0</SRCDEVICE><DSTDEVICE>1</DSTDEVICE></FRAME><COLOR>6870650</COLOR></KEYFRAME0><KEYFRAME1><TIME>4</TIME><FRAME><DSTMAC>000d.bd92.bc5b</DSTMAC><PACKET><DSTIP>192.168.1.2</DSTIP><TTL>32</TTL><PROTOCOL>0</PROTOCOL><SEGMENT><SRCPORT>57798</SRCPORT><DSTPORT>57798</DSTPORT></SEGMENT></PACKET><SRCDEVICE>0</SRCDEVICE><DSTDEVICE>1</DSTDEVICE></FRAME><COLOR>3331707</COLOR></KEYFRAME1></KEYFRAMES><DESCRIPTION></DESCRIPTION></SCENARIO1></SCENARIOS></SCENARIOSET><OPTIONS><SM>false</SM><CM>false</CM><HM>false</HM><AD>false</AD><AN>true</AN><SN>true</SN><SP>false</SP><HP>false</HP><ZM>false</ZM><LG>default</LG></OPTIONS></PACKETTRACER>