CCNA 2 – 6

CCNA 2 – 6.3.2 Routing Configuration

Objective:

- Configure routers to start a routing process
- Add networks that will be advertised

Step 1

a) Re-create the topology shown in the image above. The IP Addresses don’t need to be set for this activity.

b) Go to Options menu to make sure you are not in simple mode.

Step 2

a) Click on the Beijing Router

b) Enter the privileged EXEC mode using the right command.

c) Enter into global configuration mode.

d) Enter into the router configuration mode for the RIP routing process.

e) Use the network command to add networks 172.16.0.0 and 172.18.0.0

f) Go back to privileged EXEC mode by using the exit command.

g) Enter show run to view the current running configuration. It will show you which networks are using router rip. Networks 172.16.0.0 and 172.18.0.0 should be there if you entered the commands correctly.