Packet Tracer 3.2 Usage

Editing Other Devices

For all other devices, their configuration is relatively simple. A GUI is used in all instances, regardless of whether in Simple Mode or Console Mode.

> Clouds | In addition to basic parameters, you can also click the "Auto Config" button to generate an IP address and subnet mask for ports.
> Bridges | Bridges function like switches, except they have only two ports, no VLAN configuration, and no Cisco IOS support.
> Hubs | Hubs are simple devices without any special configurable parameters beyond Ethernet speed and duplex settlings.
> Access Points | Access points have one wireless port, and one port that can be swapped.
> Repeaters | Repeaters work like hubs, except it has only two ports.
> Servers | Servers work like PCs without the console port.
> Printers | Printers work like PCs without the console port.